IInstallation procedure

| Print out this category

IInstallation procedure
1) Open the Feeder Cover and the Middle Cover.
2) Remove the Delivery Guide while pushing the hook [A] in the direction of the arrow.
3) Remove the Stamp Cover.
1 Screw
CAUTION:
Be careful not to damage the [A] part of the Feed Guide with a screwdriver when removing the screw.
4) Install the Stamp Ink Cartridge to the Stamp Solenoid.
CAUTION:
Be sure to push the Stamp Ink Cartridge in until it clicks.
5) After installing the Stamp Solenoid, connect the connector.
1 Screw (P Tightening; M3x12)
1 Boss
6) Return the removed covers to their original positions.
Stamp Cover
Delivery Guide
Middle Cover
Feeder Cover