When Installing the Control Interface Kit-A1

| Print out this category

When Installing the Control Interface Kit-A1
1) Remove the Face Plate. (The removed Face Plate will not be used.)
2 Screws (The removed Screw will not be used.)
2) Put the CC-VI Cable through the D-SUB Support Plate.
CAUTION:
Install the extruded side of the D-SUB Support Plate as shown in the figure.
3) Connect the CC-VI Cable to the Main Controller PCB 1.
2 Hexagon Screws (Nuts will not be used.)
2 Spring Washers (Small)
2 Washers (Large)
1 Connector
NOTE:
Be sure to tighten the Hexagon Screw with needlenose pliers.