Receive/Forward

| Print out this category

Receive/Forward
* Default Setting
*1 Indicates items that appear only when the appropriate optional equipment is attached.
*7 Indicates item that is not delivered as device information.
Receive Type, Details/Edit, Delete, Print List, E-Mail Priority

Item | Setting Description | Device Information Delivery Available
Output Report
| TX/RX User Data List | Print List | No
| Fax User Data List*1 | Print List | No
Common Settings
| Print on Both Side | On, Off* | Yes
| Select Drawer |  |
|  | Switch A | On*, Off | Yes
|  | Switch B | On*, Off | Yes
|  | Switch C | On*, Off | Yes
|  | Switch D | On*, Off | Yes
| Reduce Fax RX Size | On*, Off | Yes
| On Reduction Mode: Auto Reduction %: 90% Reduction Direction: Vertical Only | Yes
| 2 On 1 Log | On, Off* | Yes
| Received Page Footer | Print, Do Not Print* | Yes
| Handle Files with Forwarding Errors | Always Print*, Store/Print, Off | Yes
| Forwarding Settings | Type, Validate/Invalidate, Register (Registered Forwarding Settings), Forward w/o Conditions, E-Mail Priority, Details/Edit, Delete, Print List | Yes*7
| Set Fax/I-Fax Inbox
|  | Set/Register Confidential Fax Inboxes
|  |  | Inbox No. | 00 to 49 | Yes
|  |  | Register Box Name: | 24 characters maximum | Yes
|  |  | PIN | Seven digits maximum | Yes
|  |  | URL Send Settings | - | Yes
|  |  | Initialize | - | No
|  | Memory RX Inbox PIN | Seven digit number | No
|  | Use Fax Memory Lock*1 | On, Off* | Yes
|  | Use I-Fax Memory Lock | On, Off* | Yes
|  | Memory Lock Start Time | Everyday, Select Days, Off* | Yes
|  | Memory Lock End Time | Everyday, Select Days, Off* | Yes
|  | Divided Data RX Timeout | 0 to 99 hours (24hours*) | Yes
| Always Send Notice for RX Errors | *On, Off | Yes
Fax Settings*1
| ECM RX | On*, Off | Yes
| Fax RX Report | For Error Only, On, Off* | Yes
| Confidential Fax Inbox RX Report | On*, Off | Yes
| RX Start Speed | 33600 bps*, 14400 bps, 9600 bps, 7200 bps, 4800 bps, 2400 bps | Yes
| RX Password | 20 digits maximum | No