FUNCTION

| Print out this category

FUNCTION

FEEDER>FUNCTION
MTR-CHK | Specifying DADF Operation Motor
Lv.1 | Details | To specify the DADF Motor to operate. The motor is activated by MTR-ON.
Use case | At operation check
Adj/set/operate method | Enter the value, and then press OK key.
Display/adj/set range | 0 to 1 0: Pickup motor (M1) 1: Release motor (M2)
Related service mode | FEEDER> FUNCTION> MTR-ON
TRY-A4 | Adj of DADF Tray width detect ref 1: A4
Lv.1 | Details | To automatically adjust the paper width detection reference point 1 for the DADF Tray. (A4)
Use case | - When replacing the Original Width Volume (VR) - When replacing the Reader Controller PCB/clearing RAM data
TRY-A5R | Adj of DADF Tray width detect ref 2: A5R
Lv.1 | Details | To automatically adjust the paper width detection reference point 2 for the DADF Tray. (A5R)
Use case | - When replacing the Original Width Volume (VR) - When replacing the Reader Controller PCB/clearing RAM data
TRY-LTR | Adj of DADF Tray width detect ref 1: LTR
Lv.1 | Details | To automatically adjust the paper width detection reference point 1 for the DADF Tray. (LTR)
Use case | - When replacing the Original Width Volume (VR) - When replacing the Reader Controller PCB/clearing RAM data
TRY-LTRR | Adj of DADF Tray width detect ref2: LTRR
Lv.1 | Details | To automatically adjust the paper width detection reference point 2 for the DADF Tray. (LTRR)
Use case | - When replacing the Original Width Volume (VR) - When replacing the Reader Controller PCB/clearing RAM data
FEED-CHK | Specifying DADF individual feed mode
Lv.1 | Details | To specify the feed mode for DADF. Feed operation is activated by FEED-ON.
Use case | At operation check
Adj/set/operate method | Enter the value, and then press OK key.
Display/adj/set range | 0 to 3 0: 1-sided pickup/delivery operation 1: 2-sided pickup/delivery operation 2: 1-sided pickup/delivery operation (with stamp) 3: 2-sided pickup/delivery operation (with stamp)
Related service mode | FEEDER> FUNCTION> FEED-ON
CL-CHK | Specifying DADF Operation Clutch
Lv.1 | Details | To specify the DADF clutch to operate. The clutch is activated by CL-ON.
Use case | At operation check
Adj/set/operate method | Enter the value, and then press OK key.
Display/adj/set range | 0 to 1 0: Paper feed clutch (CL1) 1: Registration clutch (CL2)
Related service mode | FEEDER> FUNCTION> CL-ON
CL-ON | Operation check of DADF Clutch
Lv.1 | Details | To start operation check for the clutch specified by CL-CHK
Use case | At operation check
Adj/set/operate method | 1) Select the item, and then press OK key. The unit operates for approximately 5 seconds and automatically stops. 2) Press OK key. The operation check is completed.
Required time | Approx. 5 seconds
Related service mode | FEEDER> FUNCTION>CL-CHK
FAN-CHK | Specifying DADF Operation Fan
Lv.1 | Details | To specify the DADF Fan to operate. The fan is activated by FAN-ON.
Use case | At operation check
Adj/set/operate method | Enter the value, and then press OK key.
Display/adj/set range | 0 0: Cooling Fan (FM1)
Related service mode | FEEDER> FUNCTION>FAN-ON
FAN-ON | Operation check of DADF Fan
Lv.1 | Details | To start operation check for the fan specified by FAN-CHK.
Use case | At operation check
Adj/set/operate method | 1) Select the item, and then press OK key. The unit operates for approximately 5 seconds and automatically stops. 2) Press OK key. The operation check is completed.
Required time | Approx. 5 seconds
Related service mode | FEEDER> FUNCTION> FAN-CHK
SL-CHK | Specifying DADF Operation Solenoid
Lv.1 | Details | To specify the DADF solenoid to operate. The solenoid is activated by SL-ON.
Use case | At operation check
Adj/set/operate method | Enter the value, and then press OK key.
Display/adj/set range | 0 to 1 0: Disengagement Solenoid (SL1) 1: Stamp Solenoid (SL2)
Related service mode | FEEDER> FUNCTION> SL-ON
SL-ON | Operation check of DADF Solenoid
Lv.1 | Details | To start operation check for the solenoid specified by SL-CHK.
Use case | At operation check
Adj/set/operate method | 1) Select the item, and then press OK key. The unit operates for approximately 5 seconds and automatically stops. 2) Press OK key. The operation check is completed.
Required time | Approx. 5 seconds
Related service mode | FEEDER> FUNCTION> SL-CHK
MTR-ON | Operation check of Motor
Lv.1 | Details | To start operation check for the motor specified by MTR-CHK.
Use case | At operation check
Adj/set/operate method | 1) Select the item, and then press OK key. The unit operates for approximately 5 seconds and automatically stops. 2) Press OK key. The operation check is completed.
Required time | Approx. 5 seconds
Related service mode | FEEDER> FUNCTION> MTR-CHK
ROLL-CLN | Rotation of DADF Rollers
Lv.1 | Details | To rotate for cleaning the DADF Rollers. Clean the roller by putting the lint-free paper moistened with alcohol while it is rotating.
Use case | At roller cleaning
Adj/set/operate method | 1) Select the item, and then press OK key. 2) Clean the rotating rollers with lint-free paper moistened with alcohol. 3) Press OK key. The rollers stop.
FEED-ON | Operation check of DADF individual feed
Lv.1 | Details | To start operation check for the feed mode specified by FEED-CHK.
Use case | At operation check
Adj/set/operate method | Select the item, and then press OK key.
Related service mode | FEEDER> FUNCTION> FEED-CHK