Auto Adjust Gradation

| Print out this category

Auto Adjust Gradation
1) Clean the Copyboard Glass surface of the host machine.
2) Set A3, A4, 11x17, or LTR size papers in a cassette. (Refer to the cassette settings.)
3) Select [Settings/Registration] > [Adjustment /Maintenance] > [Adjust Image Quality] > [Auto Adjust Gradation].
4) Select the source of paper for test print, and press [OK].
5) From this point on, follow the instruction on UI.