FEED-SW

| Print out this category

FEED-SW

COPIER>OPTION>FEED-SW
TFL-RTC | Set delvry dest at rcvry after tray full

Lv.1

Details

To select the delivery destination for a job with multiple pages after recovering the Delivery Tray that reaches the full level.
When 0 (default) is set, a job is output from the delivery destination again from which the last job was delivered.
When 1 is set, a job is output from the delivery destination which priority is set as high at ""Output Tray Settings"" in user mode.

Use case | When changing the delivery tray
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 0 to 1 0: Output from the tray from which the last job was output. 1: Output from the delivery destination which priority is high among the delivery trays.
Default value | 0
Related user mode | Function Settings> Common> Paper Output Settings> Output Tray Settings
SP-SW | Set separation priority mode
Lv.2 | Details | To set the separation priority mode 1 or 2 for using the thin paper of the out-of specification
Use case | When the moist, soft and thin paper is used
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 0: OFF 1: Separation priority mode 1 (Separation effect improves.) 2: Separation priority mode 2 (Separation effect improves more.)
Default value | 0
PK-SP-SW | Adj of paper feed speed
Lv.2 | Details | To set whether the acceleration process is used or the constant speed process is used in the paper feed sequence
Use case | When the acceleration process is used in the paper feed sequence
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 0: OFF 1: ON
Default value | 0