Installation to the Host Machine

| Print out this category

Installation to the Host Machine
1) Install the Option HDD to the HDD Fixation Plate.
2 Screws (TP; M3X6) (enclosed with option HDD)
2) Return the HDD Fixation Plate Unit to the HDD Box.
3) Install the HDD Box to the HDD Slide Rail.
4) Return the HDD Unit to the host machine.
NOTE:
Be sure to move the unit in the direction of the arrow when installing it to prevent the protrusion of the HDD Slide Rail from coming in contact with the plate of the host machine.
Be sure not to push the cable in the host machine.
5) Connect the 2 connectors.
1 Wire Saddle
NOTE:
When connecting the connector, be sure to connect it with the terminals inside the connector is on the rear side.
Be sure to pass the cable through the Wire Saddle when connecting.
6) Secure the HDD Unit.
2 Screws (Use the screws removed in "Removing the HDD" step 8.)
CAUTION:
Be careful not to drop the screw.
Be sure to tighten the screws in the order shown in the figure.
7) Close the plate.
8) Insert the Main Controller PCB 1 until it stops. (2 Screws)
CAUTION:
Be sure to install the Main Controller PCB 1 while paying attention not to trap cables.
Check that the Main Controller PCB 1 is installed properly.
9) Connect the USB Cable and the Control Panel Communication Cable.
10) Install the covers.
Controller Box Cover
Rear Cover (4 Screws) (Tighten the screws in the following order: upper left, lower left, upper right, and then lower right.)
Right Rear Cover (2 Screws)
NOTE:
When installing the Right Cover (Upper Rear), open the Right Cover to make the work easier.