Left Edge Margin Adjustment (2nd side)

| Print out this category

Left Edge Margin Adjustment (2nd side)
NOTE:
By executing the margin adjustment (2nd side) for the Cassette 1, the adjustment is applied to all source of paper.
Execute duplex printing from the Cassette 1, and check that the left edge margin is within 2.5
+/- 2.0mm.
If it is not within the range, execute adjustment by following the procedure below.
1) Adjust the image position in service mode.
Service mode (Level 1) > COPIER > ADJUST > FEED-ADJ > ADJ-REFE
NOTE:
<Setting Range>
-128 to 127 (0.1mm per unit)
As the value is incremented by 1, the left edge margin is increased by 0.1mm.
2) Execute duplex printing from the Cassette 1, and check that the left edge margin is within 2.5 +/- 2.0mm.
3) When the setting value was changed in step 1), write down the new numerical value in the service label.
4) Exit from the service mode.