Installation Procedure

| Print out this category

Installation Procedure
1) Release the interface cable from the wire saddle, and then disconnect the paper deck connector from the host machine.
2) Release the paper deck from the host machine, and then press down the latch plate of the paper deck to open the compartment.
3) Detach the right cover of the paper deck in the direction of the arrow shown.
3 Screws
4) Detach the rear cover of the paper deck.
6 Screws (M4x8: 4 pcs., M3x8: 2 pcs.)
NOTE:
When the rear cover is removed, loosen the screw shown by an arrow in the figure, if it is difficult to remove the rear cover because of contacting to the left rear cover.
5) Detach the front upper cover.
3 Screws
1 Connector
6) Detach the top cover.
2 Screws
7) Attach the supplied cable protection bushing to the hole on the top panel of the paper deck.
8) Place the heater unit under the top panel of the paper deck, and then take the connector out of the hole on the top plate.
9) Insert the 2 hooks of the heater unit into the holes on the top plate of the paper deck, and then secure the heater unit to the main body of the paper deck.
1 Screw (w/washer; M4x8)
10)Attach the heater connector to the panel mount.
11)Remove the blindfold plate from the power cord mount of the paper deck.
1 Screw
NOTE:
Removed screw and blindfold cover are no longer reused.
12)Install the supplied AC input connector in order of [A] -> [B].
13)Attach the 5 wire saddles (black) to the rear side panel of the paper deck as shown.
14)Put the relay harness in the 5 wire saddles (black), and then attach the connector.
NOTE:
2 snap-bands (A) equipped with the relay harness are not used.
15)Put the relay harness in the 2 wire saddles on the power cord mount, and then connect the connector.
16)Reattach the external covers of the paper deck in the following sequence:
[1] Top cover (2 screws; M4x8)
[2] Right cover (3 screws; M4x8)
[3] Rear cover (4 screws; M4x8 and 2 screws; M3x8)
[4] Front upper cover (1 connector and 2 screws; M4X8)
17)Manually slide the paper deck to the left to place it aside of the host machine
18)Remove the connector cover at the rear side of the host machine. And then disconnect 3 connectors for the cassette pedestal.
1 Screw
19)Remove the lower rear cover, and then cut out the blindfold cover with the nipper.
4 Screws
20)Attach the connector of the AC output connector to the heater PCB, insert the AC output connector and then fasten the ground cable.
1 Screw (Binding; M4x6)
1 Toothed washer
21)Reattach the external covers of the host machine in the following sequence:
[1] Lower rear cover (4 screws; M3x8)
[2] Connector cover (3 connctors and 1 screw; M3x8)
22)Put the interface cable of the paper deck in the wire saddle and then connect the connector of the paper deck to the back of the host machine. Detach the 2 blindfold seals from the rear cover of the host machine, and then attach the 2 wire saddles (white).
23)Connect the connector of the supplied AC connector to the power cord mount of the heater. Put the AC cable in the wire saddles, and then connect the other connector (plug) to the receptacle of the host machine.
24)Fix the supplied plug cover at rear side of the host machine.
1 Screw (Binding; M4x4)
25)Stick the supplied power supply label to the rear cover of the paper deck.