Downloading System Software (Confirmation)

| Print out this category

Downloading System Software (Confirmation)
[2]: Upgrade (w Confirmation)
The version is compared between the host machine/option and the system software in the USB memory storage device to download the system software with newer version in the USB memory storage device to the temporary storage area of the HDD.
When the system software version in the USB memory storage device is the same or older, a confirmation message is displayed on the Control Panel so that the user can select whether to overwrite or not.
In safe mode, only the following system software can retrieve the version information (the version is compared).
SYSTEM, LANGUAGE, RUI, MERAPCONT, SDICT
As for system software of the host machine whose version information cannot be obtained, the software for RCON is not downloaded, but other software are downloaded.
For the system software of the option that is not connected, it is handled as follows:
<In the case of startup in normal mode (Recommended)>
For the option that is not connected, the system software is not to be downloaded.
<In the case of startup in safe mode>
The system software of the options which are not connected are not downloaded.
Unlike menu [1], this machine is not automatically started despite completion of downloading. By manually turning OFF/ON the power, the system software is written at the time of startup.In this case, starting the machine in safe mode deletes the downloaded system software saved in the temporary storage area; therefore, do not press the numeric keys (2 + 8), but execute normal startup to execute writing.
Operation procedure
1) Enter download mode.
2) Connect the USB memory storage device to the USB port.
3) Press the key on the Control Panel.
[2] -> [0]: To execute downloading/Any key other than [0] key: To return to the menu screen.
During downloading, download status is displayed on the Control Panel.
NOTE:
When the system software version in the USB memory storage device is the same or older than the system software in the HDD, a message is displayed in each case to confirm whether to overwrite or not.
Press the key on the Control Panel.
[0]: To overwrite/Any key other than [0]: Not to overwrite
Once downloading is complete, a message is displayed to encourage pressing the “Reset” key.
4) Press the “Reset” key.
Shutdown sequence is executed.
5) Once the message on the touch panel disappears, turn OFF the Main Power Switch.
6) Remove the USB memory storage device.
7) Ensure the LED at the lower right on the Control Panel is turned OFF, and turn ON the Main Power Switch.
Writing to the HDD system area/flash ROM is started after the startup. The screen shows the countdown once the writing process is properly completed.
The screen shows the countdown once the writing process is properly completed. This machine is restarted with the downloaded system software at the count of 0.