Affixing the ADF Label (only for the standard model with an ADF)

| Print out this category

Affixing the ADF Label (only for the standard model with an ADF)
1) If the following labels are supplied, go through the steps described below.
Finger pinch caution label 1
Finger pinch caution label 2
2) Affix the finger pinch caution label 1 written in an appropriate language to the existing label.

3) Open the DADF.
4) Affix the finger pinch caution label 2 written in an appropriate language to the existing label..