Setting after installation

| Print out this category

Setting after installation
1) Turn on the main power switch.
2) Enter in the service mode.
3) COPIER > OPTION > ACC > choose IN-TRAY and register "1".
4) Do OFF/ON of the main power supply.
5) [ Settings / Registration] > [ Function settings] > [ Common] > [ Paper output settings] > [ Output Tray settings] of confirm that a menu is added.
6) Select copy to the Tray B, and perform test copy.
7) Check that a copy is delivered to the Inner 2way Tray.
8) Set the tray in accordance with user’s request.