Confirmation and preparation in advance

| Print out this category

E-RDS Setup
Confirmation and preparation in advance
To monitor a device with e-Maintenance/ imageWARE Remote, the following settings are required.
(1) Advance confirmation
Confirm with the UGW administrator that the device to be monitored with e-Maintenance/ imageWARE Remote is registered in the UGW.
(2) Advance preparations
Interview the user’s system administrator in advance to find out the following information about the network.
Information item 1
IP address settings
Automatic setting : DHCP, RARP, BOOTP
Manual setting : IP address, subnet mask and gateway address to be set
Information item 2
Is there a DNS server in use?
If there is a DNS server in use, find out the following.
Primary DNS server address
Secondary DNS server address
Information item 3
Is there a proxy server?
If there is a proxy server in use, find out the following.
Proxy server address
Port No. for proxy server
Information item 4
Is proxy server authentication required?
If proxy server authentication is required, find out the following.
User name and password required for proxy authentication
(3) Network settings
Based on the results of the information obtained in (2) Advance preparations, make the device network related settings in accordance with the following procedures.
1) Displaying the Settings/ Registration screen
1. Touch the [Settings/Registration (User Mode)] button.
2. When a system management department ID and system management password are set up, touch the [Log In] button and enter the System Management ID and System PIN to perform a log-in.
2) Setting IP address-related items (* In case of IPv4 )
1. Touch the [Preferences] > [Network] > [TCP/IP Settings] > [IPv4 Settings] > [IP Address Settings] buttons.
2. Set the IP address based on the result obtained in “(2) Advance preparations - Information item 1”, and touch the [OK] button.
For automatic acquisition, select from [DHCP], [RARP], [BOOTP].
For manual setting, set the IP address, subnet mask and gateway address.
3. When DNS settings and proxy settings are not made, touch the [Close] button to reboot the device.
3) DNS Settings
1. Select [TCP/IP Settings] from breadcrumbs of the left columns, and then Touch it.
2. Touch the [TCP/IP Settings] > [DNS Settings] > [DNS Server Address Settings] buttons.
3. Set the DNS server address based on the result obtained in “(2) Advance preparations - Information item 2” and touch the [OK] button.
Select [Primary DNS Server] and make settings.
When the secondary DNS server is installed, select [Secondary DNS Server] and make settings.
4. When proxy settings are not made, touch the [Close] button to reboot the device.
4) Proxy Settings
1. Select [TCP/IP Settings] from breadcrumbs of the left columns, and then Touch it.
2. Touch the [TCP/IP Settings] > [Proxy Settings].
3. Set the proxy server based on the result obtained in “(2) Advance preparations - Information item 3”.
a) Use Proxy to [On].
b) Enter the server address.
c) Enter port Number (Validation: 1 to 65,535).
d) If proxy server authentication is required, Touch [Set Authentication].(see figure above)
e) Set the following items based on the result obtained in “(2) Advance preparations - Information item 4”.
Set Use Proxy Authentication to [On].
Enter User name and Password, and touch the [OK] button.
f) Touch the [OK] button.
4. Touch the [Close] button.
5. Reboot the device.
CAUTION:
When changes are made to the above-mentioned network settings, be sure to reboot the device.