Location code

| Print out this category

Location code
Error code, jam code, and alarm code include the location information.
Location information is displayed as 2-digit numbers as follows.

Device | JAM | ERR | ALARM
imageRUNNER ADVANCE 4051/4045/4035/4025 Series | Printer engine = 00 ADF=01 | Main Controller = 00 Reader+ADF=04 Printer engine = 05 | Others of listed below
Image Reader Unit-E1 DADF-AG1 | ADF=01 | Reader+ADF=04 | 02
Paper Deck Unit-B2 | 00 | 05 | 04
Cassette Feeding Unit-AF1 | 00 | 05 | -
Buffer Pass Unit-H1 | 00 | 05 | -
Staple Finisher-G1/Booklet Finisher-G1 | 02 | 02 | 61, 62
External 2, 2/3, 2/4, 4 Hole Puncher-B2 | 02 | 02 | 65
Inner Finisher-D1 | 02 | 02 | 61, 62
Inner 2, 2/3, 2/4, 4 Hole Puncher-A1 | 02 | 02 | 65