PART-CHK

| Print out this category

PART-CHK

COPIER>FUNCTION>PART-CHK
CL | Specification of operation Clutch
Lv.1 | Details | To specify the Clutch to operate.
Use case | When replacing the Clutch/checking the operation
Adj/set/operate method | Enter the value, and then press OK key.

Display/adj/set range

1 to 6
1:Manual feed pickup clutch (CL12)
2:Registration clutch (CL3)
3:Developing cylinder clutch (CL1)
4:Not used
5:Not used
6:Deck pickup clutch (CL2D)

Related service mode | COPIER> FUNCTION> PART-CHK> CL-ON
CL-ON | Operation check of Clutch
Lv.1 | Details | To start operation check of the Clutch specified by CL. The operation stops after ""ON for 0.5 sec"" => ""OFF for 10 sec"" => ""ON for 0.5 sec"" => ""OFF for 10 sec"" => ""ON for 0.5 sec"".
Use case | When replacing the Clutch/checking the operation
Adj/set/operate method | Select the item, and then press OK key.
Display/adj/set range | During operation: ACTIVE, When operation finished normally: OK!
Default value | 0
Required time | Approx. 22 seconds
Related service mode | COPIER> FUNCTION> PART-CHK> CL
MTR | Specification of operation Motor
Lv.1 | Details | To specify the Motor to operate.
Use case | When replacing the Motor/checking the operation
Adj/set/operate method | Enter the value, and then press OK key.
Caution | Be sure to remove the Toner Container before Bottle motor (M17) is activated. If it remains to be installed, toner is supplied.

Display/adj/set range

1 to 16
1:Polygon motor (M11)
2:Main motor (M1)
3:Fixing motor (M2)
4:No.1 delivery motor (M10)
5:Bottle motor (M17)
6:Cassette 1 pickup motor (M13)
7:Cassette 2 pickup motor (M3)
8:Duplex feed motor (M9)
9:Hopper motor(M16)
10:Cassette 3 pickup motor
11:Cassette 4 pickup motor
12:Deck open solenoid (M1D)
13:Deck lifter motor (M2D)
14:Reversal motor(M20)
15:Not used
16:Buffer pass motor (M101)

Related service mode | COPIER> FUNCTION> PART-CHK> MTR-ON
MTR-ON | Operation check of Motor
Lv.1 | Details | To start operation check of the Motor specified by MTR. The operation automatically stops after operation of 20 seconds.
Use case | When replacing the Motor/checking the operation
Adj/set/operate method | Select the item, and then press OK key.
Caution | Be sure to remove the Toner Container before Toner Supply Motor (M10) is activated. If it remains to be installed, toner is supplied.
Display/adj/set range | During operation: ACTIVE, When operation finished normally: OK!
Required time | 1 minute
Related service mode | COPIER> FUNCTION> PART-CHK> MTR
SL | Specification of operation Solenoid
Lv.1 | Details | To specify the Solenoid to operate.
Use case | When replacing the Solenoid/checking the operation
Adj/set/operate method | Enter the value, and then press OK key.

Display/adj/set range

1 to 10
1:Cassette 1 pickup solenoid (SL1)
2:Cassette 2 pickup solenoid (SL2)
3:Cassette 3 pickup solenoid
4:Cassette 4 pickup solenoid
5:Deck pickup roller release solenoid (SL1D)
6:Deck open solenoid (SL2D)
7:Reversal Solenoid (SL12)
8:No. 2 Delivery Solenoid (SL13)
9:Not used
10:Manual feed pickup solenoid (SL2)

Related service mode | COPIER> FUNCTION> PART-CHK> SL-ON
SL-ON | Operation check of Solenoid
Lv.1 | Details | To start operation check for the Solenoid specified by SL. The operation stops after ""ON for 0.5 sec"" => ""OFF for 10 sec"" => ""ON for 0.5 sec"" => ""OFF for 10 sec"" => ""ON for 0.5 sec"".
Use case | When replacing the Solenoid/checking the operation
Adj/set/operate method | Select the item, and then press OK key.
Display/adj/set range | During operation: ACTIVE, When operation finished normally: OK!
Required time | 1 minute
Related service mode | COPIER> FUNCTION> PART-CHK> SL