MISC

| Print out this category

MISC

COPIER>ADJUST>MISC
SEG-ADJ | Set criteria for text/photo: front side
Lv.1 | Details | To set the judgment level of text/photo original in Text/Photo/Map mode. As the value is increased, the original tends to be detected as a photo document, and as the value is decreased, the original tends to be detected as a text document.
Use case | When adjusting the classification level of text and photo in Text/Photo/Map mode
Adj/set/operate method | 1) Enter the setting value (switch negative/positive by -/+ key) and press OK key. 2) Turn OFF/ON the main power switch.
Caution | Do not use this at the normal service.
Display/adj/set range | -4 to 4
Default value | 0
K-ADJ | Set criteria for black text: front side
Lv.1 | Details | To set the judgment level of black characters at text processing. As the value is increased, the text tends to be detected as black.
Use case | When preferring the text to be judged as black
Adj/set/operate method | 1) Enter the setting value (switch negative/positive by -/+ key) and press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | -3 to 3
Default value | 0
ACS-ADJ | Set criteria for B&W/color in ACS:front
Lv.1 | Details | To set the judgment level of B&W/color original in ACS mode. As the value is increased, the original tends to be detected as a B&W document, and as the value is decreased, the original tends to be detected as a color document.
Use case | When adjusting the color detection level in ACS mode
Adj/set/operate method | 1) Enter the setting value (switch negative/positive by -/+ key) and press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | -3 to 3
Default value | 0
ACS-EN | Set judgment area in ACS mode:front side
Lv.1 | Details | To set the judgment area in ACS mode. As the greater value is set, the judgment area is widened.
Use case | When adjusting the judgment area in ACS mode
Adj/set/operate method | 1) Enter the setting value (switch negative/positive by -/+ key) and press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | -2 to 2
Default value | 1
ACS-CNT | Set jdgmt pixel count area in ACS:front
Lv.1 | Details | To set the area which counts the pixel to judge the color presence in ACS mode. As the greater value is set, the judgment area is widened.
Use case | When adjusting the area which counts the pixel to judge the color presence in ACS mode
Adj/set/operate method | 1) Enter the setting value (switch negative/positive by -/+ key) and press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | -2 to 2
Default value | 0
C1-ADJ-Y | Enter Cassette1 side register adj value
Lv.1 | Details | As the value is incremented by 1, the margin on the left edge of paper is increased by 0.1 mm. +: Left margin becomes smaller. (An image moves to the left.) -: Left margin becomes larger. (An image moves to the right.)
Use case | When adjusting side registration of paper picked up from Cassette 1, when executing RAM clear of the DC Controller PCB, or when replacing the PCB (Enter the value of service label.)
Adj/set/operate method | 1) Enter the setting value (switch negative/positive by -/+ key) and press OK key. 2) Turn OFF/ON the main power switch.
Caution | Be sure to enter the adjustment value on the service label after adjustment.
Display/adj/set range | -128 to +127
C2-ADJ-Y | Enter Cassette2 side register adj value
Lv.1 | Details | As the value is incremented by 1, the margin on the left edge of paper is increased by 0.1 mm. +: Left margin becomes smaller. (An image moves to the left.) -: Left margin becomes larger. (An image moves to the right.)
Use case | When adjusting side registration of paper picked up from Cassette 2, when executing RAM clear of the DC Controller PCB, or when replacing the PCB (Enter the value of service label.)
Adj/set/operate method | 1) Enter the setting value (switch negative/positive by -/+ key) and press OK key. 2) Turn OFF/ON the main power switch.
Caution | Be sure to enter the adjustment value on the service label after adjustment.
Display/adj/set range | -128 to +127
C3-ADJ-Y | Enter Cassette3 side register adj value
Lv.1 | Details | As the value is incremented by 1, the margin on the left edge of paper is increased by 0.1 mm. +: Left margin becomes smaller. (An image moves to the left.) -: Left margin becomes larger. (An image moves to the right.)
Use case | When adjusting side registration of paper picked up from Cassette 3, when executing RAM clear of the DC Controller PCB, or when replacing the PCB (Enter the value of service label.)
Adj/set/operate method | 1) Enter the setting value (switch negative/positive by -/+ key) and press OK key. 2) Turn OFF/ON the main power switch.
Caution | Be sure to enter the adjustment value on the service label after adjustment.
Display/adj/set range | -128 to +127
Default value | 0
C4-ADJ-Y | Enter Cassette4 side register adj value
Lv.1 | Details | As the value is incremented by 1, the margin on the left edge of paper is increased by 0.1 mm. +: Left margin becomes smaller. (An image moves to the left.) -: Left margin becomes larger. (An image moves to the right.)
Use case | When adjusting side registration of paper picked up from Cassette 4, when executing RAM clear of the DC Controller PCB, or when replacing the PCB (Enter the value of service label.)
Adj/set/operate method | 1) Enter the setting value (switch negative/positive by -/+ key) and press OK key. 2) Turn OFF/ON the main power switch.
Caution | Be sure to enter the adjustment value on the service label after adjustment.
Display/adj/set range | -128 to +127
Default value | 0
MF-ADJ-Y | Enter MP Tray side register adj value
Lv.1 | Details | As the value is incremented by 1, the margin on the left edge of paper is increased by 0.1 mm. +: Left margin becomes smaller. (An image moves to the left.) -: Left margin becomes larger. (An image moves to the right.)
Use case | When adjusting side registration of paper picked up from Multi-purpose Tray, when executing RAM clear of the DC Controller PCB, or when replacing the PCB (Enter the value of service label.)
Adj/set/operate method | 1) Enter the setting value (switch negative/positive by -/+ key) and press OK key. 2) Turn OFF/ON the main power switch.
Caution | Be sure to enter the adjustment value on the service label after adjustment.
Display/adj/set range | -128 to +127
Default value | 0
DK-ADJ-Y | Enter Paper Deck side register adj value
Lv.1 | Details | As the value is incremented by 1, the margin on the left edge of paper is increased by 0.1 mm. +: Left margin becomes smaller. (An image moves to the left.) -: Left margin becomes larger. (An image moves to the right.)
Use case | When adjusting side registration of paper picked up from Paper Deck, when executing RAM clear of the DC Controller PCB, or when replacing the PCB (Enter the value of service label.)
Adj/set/operate method | 1) Enter the setting value (switch negative/positive by -/+ key) and press OK key. 2) Turn OFF/ON the main power switch.
Caution | Be sure to enter the adjustment value on the service label after adjustment.
Display/adj/set range | -128 to +127
Default value | 0
ACS-EN2 | Set ACS mode jdgmt area in DADF mode
Lv.1 | Details | To set the judgment area in ACS mode at DADF reading. As the greater value is set, the judgment area is widened.
Use case | When adjusting the judgment area in ACS mode at DADF reading
Adj/set/operate method | 1) Enter the setting value (switch negative/positive by -/+ key) and press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | -2 to 2
Default value | 1
ACS-CNT2 | Set ACS jdgmt pixel count area in DADF
Lv.1 | Details | To set the area which counts the pixel to judge the color presence in ACS mode at DADF reading. As the greater value is set, the judgment area is widened.
Use case | When adjusting the area which counts the pixel to judge the color presence in ACS mode at DADF reading
Adj/set/operate method | 1) Enter the setting value (switch negative/positive by -/+ key) and press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | -2 to 2
Default value | 0
TBSIS-WB | Setting of blank band ejection time
Lv.1 | Details | To set the blank band ejection time. As the value is incremented by 1, the ejection time changes by 0.1 second. +: Increase -: Decrease
Use case | When an image failure (streaks of uneven density) occurs
Adj/set/operate method | Enter the setting value (switch negative/positive by -/+ key) and press OK key.
Caution | When a positive value is set, the ejection time increases.
Display/adj/set range | -2 to 2
Default value | 0
DCON-V | Fine adj DC Controller reference voltage
Lv.1 | Details | To make a fine adjustment of the reference voltage of CPU drive voltage (3.3V) on the DC Controller PCB.
Use case | When the reference voltage is deviated from the center value (3.41 V) significantly
Adj/set/operate method | Enter the setting value (switch negative/positive by -/+ key) and press OK key.
Caution | Because it affects the scanning values of the Potential Sensor and Patch Sensor, image density may vary.
Display/adj/set range | -14 to 14
Default value | 0
HP-OFST | Setting of 2D shading drum HP offset
Lv.1 | Details | To set the home position of Photosensitive Drum in the vertical scanning direction at 2D shading. As the value is incremented by 1, the home position moves by 10 mm.
Use case | When adjusting the home position of the Photosensitive Drum at the replacement of the drum
Adj/set/operate method | Enter the setting value (switch negative/positive by -/+ key) and press OK key.
Display/adj/set range | -5 to 5
Default value | 0