Scanner Motor Control

| Print out this category

Scanner Motor Control
1) Forward movement when scanning an image
CCD operation is controlled by the following sensors when scanning the image.
NOTE:
The scanning speed of this machine is as follows.
Black/white (600dpi x 600dpi):260 mm/sec
Color SEND(600dpi x 300dpi):140 mm/sec
2) Backward movement after scanning an image
After scanning an image, CCD moves backward to CCD shading position at a specific speed (260 mm/sec).