Required Options and Conditions

| Print out this category

Scanning System Options
Required Options and Conditions

Product name | Required options, conditions, etc.
DADF-AG1 | Paper weight: <1-sided> AB configuration: 42 to 128 g/m2, Inch configuration: 50 to 128 g/m2 <2-sided> 50 to 128 g/m2 Stacking capacity: 100 sheets (50 to 80 g/m2)
Platen Cover Type R |
ADF Access Handle-A1 | It is the cover to be installed at the top of the host machine when using this equipment as a printer model.
Stamp Unit-B1 | Option for ADF
Reader Heater Unit-H1 | For 200V Use it to suppress the dew condensation in the reader unit. Heater Kit-K1 is required.
Color Image Reader Unit-E1 | ADF+Reader EU only
Printer Cover-C1 | It is the handle to support opening and closing the Feeder. EU only