SYSTEM

| Print out this category

SYSTEM

COPIER>FUNCTION>SYSTEM
DOWNLOAD | Shift to download mode
Lv.1 | Details | To make the machine enter the download mode and wait for a command. Perform downloading by SST/USB.
Use case | At upgrade
Adj/set/operate method | 1) Select the item, and then press OK key. 2) Perform downloading by SST/USB.
Supplement/memo | SST: Service Support Tool
CHK-TYPE | HD-CLEAR/HD-CHECK exe partition No.
Lv.1 | Details | To specify the partition number of the HDD to execute HD-CLEAR/HD-CHECK.
Use case | When executing HD-CLEAR/HD-CHECK
Adj/set/operate method | Enter the value, and then press OK key.

Display/adj/set range

0 to 65535
0: Entire HDD
1: Image accumulation area
2: Universal file storage area
3: PDL file storage area
4: Program file storage area
5: MEAP application
6: Address book transfer setting
7: MEAP storage data
8: System log storage area
9: Advanced Box area
10: Area for distribution server
11: Storage area of universal data

Related service mode | COPIER> FUNCTION> SYSTEM> HD-CLEAR, HD-CHECK
Supplement/memo | Universal file: Management information of user setting data, various log data, PDL spool data, and image data, etc.
HD-CHECK | Entire HDD check and recovery
Lv.1 | Details | To check the entire HDD and execute recovery processing.
Adj/set/operate method | Select the item, and then press OK key.
Caution | Be sure to execute this item after CHK-TYPE.
Display/adj/set range | During operation: Progress ratio (%), When operation finished normally: OK!
Related service mode | COPIER> FUNCTION> SYSTEM> CHK-TYPE
HD-CLEAR | Initialization of specified partition
Lv.1 | Details | To initialize the HDD partition specified by CHK-TYPE.
Use case | When initializing the HDD partition
Adj/set/operate method | Select the item, and then press OK key.
Caution | Be sure to execute this item after CHK-TYPE.
Display/adj/set range | When operation finished: OK!/NG!
Related service mode | COPIER> FUNCTION> SYSTEM> CHK-TYPE
DEBUG-1 | Setting of log type and save timing
Lv.2 | Details | To set the types of logs to be stored and the timing to store logs in the HDD. Logs are used to analyze the cause of a trouble.
Use case | When analyzing the cause of a problem
Adj/set/operate method | Select the item, and then press OK key.
Caution | Do not use this at the normal service. Change the setting value in accordance with the instructions from the Quality Support Division.
Display/adj/set range | 0 to 3 0: Save PLOG at detection of Reboot/Exception 1: Save PLOG at detection of Reboot/Exception/Encode 2: Save SUBLOG at detection of Reboot/Exception/Encode 3: Save SUBLOG in overwrite mode at detection of Reboot/Exception/Encode
Default value | 3
Related service mode | COPIER> FUNCTION> SYSTEM> DEBUG-2 (Level 2)
Supplement/memo | PLOG can be printed by COPIER> FUNCTION> SYSTEM> DEBUG-2. SUBLOG cannot be printed. (It should be uploaded from SST/USB.)
DEBUG-2 | Output of log saved on HDD
Lv.2 | Details | To print the PLOG saved in HDD by COPIER> FUNCTION> SYSTEM> DEBUG-1. (A4: Approx. 20 sheets) SUBLOG is not printed. It should be uploaded from SST/USB.
Use case | When printing PLOG
Adj/set/operate method | Select the item, and then press OK key.
Caution | Do not use this at the normal service.
Display/adj/set range | During operation: ACTIVE, When operation finished normally: OK!
Related service mode | COPIER> FUNCTION> SYSTEM> DEBUG-1 (Level 2)
DSRAMBUP | Backup of DC Controller PCB SRAM
Lv.2 | Details | To back up the setting data in SRAM of the DC Controller PCB.
Use case | When replacing the DC Controller PCB for troubleshooting at the time of trouble occurrence
Caution | During operation, the setting data changes by manual or automatic adjustment. When backup data which has been left for a long period of time is restored, it is overwritten with new setting data and the old data is deleted.
Related service mode | COPIER> FUNCTION> SYSTEM> DSRAMRES
DSRAMRES | Restore of DC Controller PCB SRAM
Lv.2 | Details | To restore the setting data which has been backed up in SRAM of the DC Controller PCB.
Use case | When replacing the DC Controller PCB for troubleshooting at the time of trouble occurrence
Caution | During operation, the setting data changes by manual or automatic adjustment. When backup data which has been left for a long period of time is restored, it is overwritten with new setting data and the old data is deleted.
Related service mode | COPIER> FUNCTION> SYSTEM> DSRAMBUP
RSRAMBUP | Backup of CCD unit (CCD PCB) SRAM
Lv.2 | Details | To back up the setting data in SRAM of the CCD unit (CCD PCB).
Use case | When replacing the CCD unit (CCD PCB) for troubleshooting at the time of trouble occurrence
Caution | During operation, the setting data changes by manual or automatic adjustment. When backup data which has been left for a long period of time is restored, it is overwritten with new setting data and the old data is deleted.
Related service mode | COPIER> FUNCTION> SYSTEM> RSRAMRES
RSRAMRES | Restore of CCD unit (CCD PCB) SRAM
Lv.2 | Details | To restore the setting data which has been backed up in SRAM of the CCD unit (CCD PCB).
Use case | When replacing the CCD unit (CCD PCB) for troubleshooting at the time of trouble occurrence
Caution | During operation, the setting data changes by manual or automatic adjustment. When backup data which has been left for a long period of time is restored, it is overwritten with new setting data and the old data is deleted.
Related service mode | COPIER> FUNCTION> SYSTEM> RSRAMBUP
R-REBOOT | Reboot of the device
Lv.1 | Details | Perform the reboot from the service mode
Use case | When the reboot is carried out with the remote control by VNC