DEVELOP

| Print out this category

DEVELOP

COPIER>ADJUST>DEVELOP
DE-OFST | Entering the offset value for the developing DC bias
Lv.1 | Use case | When the abnormal image appears (high or low density)
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Caution | The density becomes high by increasing the value. After the setting value is changed, write the changed value in the service label.
Display/adj/set range | -128 to 127
Default value | 0