ACC-STS

| Print out this category

ACC-STS

COPIER>DISPLAY>ACC-STS
FEEDER | Display of DADF connection state
Lv.1 | Details | To display the connecting state of DADF.
Use case | When checking the connection between the machine and DADF
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 0 to 1 0: Not connected, 1: Connected
SORTER | Display of connect state of Finisher-related option
Lv.1 | Details | To display the connecting state of Finisher-related options.
Use case | When checking the connection of Finisher-related options
Adj/set/operate method | N/A (Display only)

Display/adj/set range

Left column (connecting state of Finisher-related options): 1 to 5
1: Without Saddle
2: With Saddle, without Folding Unit
3: With Saddle and Inserter, without Folding Unit
4: With Saddle and Folding Unit, without Inserter
5: With Saddle, Inserter and Folding Unit
Right column (connecting state of Finisher-belonged Inserter): 0 to 4
0: no hole, 1: 2-hole, 2: 2/3-hole, 3: 4-hole, 4: 4-hole (SW)

DECK | Display of Paper Deck connection state
Lv.1 | Details | To display the connecting state of the Paper Deck.
Use case | When checking the connection between the machine and the Paper Decks
Adj/set/operate method | N/A (Display only)

Display/adj/set range

0 to 8
0: Not connected
1: Connected (small) (Display is hidden on this machine.)
2: Connected (large)
3: POD Deck Lite (with Multi-purpose Tray)
4: POD Deck Lite (without Multi-purpose Tray )
5: Multi-purpose Tray only
6: POD deck
7: 2-POD deck connected
8: 3-POD deck connected (Display is hidden on this machine.)

CARD | Dis of connection state of Card Reader
Lv.1 | Details | To display the connecting state of Card Reader.
Use case | When checking the connection between the machine and the Card Reader
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 0 to 1 0: No card is inserted while the Card Reader is connected. (Copy is not available.) 1: Card Reader is not connected, or card is inserted while the Card Reader is connected. (Copy is available.)
DATA-CON | Display of NE Controller connection state
Lv.1 | Details | To display the connecting state of NE Controller.
Use case | When checking the connection between the machine and the NE Controller
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 0 to 1 0: Not connected, 1: Connected
RAM | Display of MNCON PCB memory capacity
Lv.1 | Details | To display the memory capacity of the Main Controller PCB.
Use case | When checking the memory capacity of the machine
Adj/set/operate method | N/A (Display only)
Unit | MB
Default value | 256
COINROBO | Display of Coin Manager connection state
Lv.1 | Details | To display the connecting state of the Coin Manager.
Use case | When checking the connection between the machine and the Coin Manager
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 0 to 1 0: Not connected, 1: Connected
NIB | Display of Network PCB connection state
Lv.1 | Details | To display the connecting state of the Network PCB.
Use case | When checking the connection between the machine and the Network PCB
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 0 to 3 0: Not connected, 1: Ethernet PCB connected, 2: Token Ring PCB connected, 3: Ethernet PCB + Token Ring PCB connected
PS/PCL | Display of PS/PCL firmware install state
Lv.1 | Details | To display the installation state of PS/PCL firmware.
Use case | When checking whether NetWare firmware is installed to the machine
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 0 to 2 0: Not installed, 1: PS/PCL, 2: PS Kanji
NETWARE | Display of NetWare firmware install state
Lv.1 | Details | To display the installation state of the NetWare firmware.
Use case | When checking whether NetWare firmware is installed to the machine
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 0 to 1 0: Not installed, 1: Installed
SEND | Display of SEND support PCB existence
Lv.1 | Details | To display whether there is PCB to support SEND function. SEND function can be used only when the PCB is mounted.
Use case | When checking the connection between the machine and the PCB that supports SEND function
Adj/set/operate method | N/A (Display only)
Display/adj/set range | 0 to 1 0: Not connected, 1: Connected
HDD | Display of HDD model name
Lv.1 | Details | To display the model name of HDD.
Use case | When checking the model name of HDD used on the machine
Adj/set/operate method | N/A (Display only)
PCI1 | Display of PCI1-connected PCB name
Lv.1 | Details | To display the name of the PCB that is connected to PCI1.
Use case | When checking the name of the PCB that is connected to PCI1
Adj/set/operate method | N/A (Display only)
Display/adj/set range | -: No PCB connected Wireless LAN Board: Wireless LAN Board
PCI2 | [Not used]
PCI3 | [Not used]
IA-RAM | Display of MNCON PCB memory(IA) capacity
Lv.1 | Details | To display the memory (IA) capacity of the Main Controller PCB.
Use case | When checking the memory capacity of the Main Controller PCB
Adj/set/operate method | N/A (Display only)
Unit | MB
Default value | 1024