FEED-ADJ

| Print out this category

FEED-ADJ

COPIER>ADJUST>FEED-ADJ
REGIST | Adj of registration start timing: Plain

Lv.1

Details

To adjust the timing to turn ON the Registration Motor in the case of plain paper.
As the value is incremented by 1, the margin on the leading edge of paper is increased by 0.1 mm.
+: Top margin becomes smaller. (An image moves upward.)
-: Top margin becomes larger. (An image moves downward.)
When replacing the DC Controller PCB/clearing RAM data, enter the value of service label.

Use case | When replacing the DC Controller PCB/clearing RAM data
Adj/set/operate method | Enter the setting value (switch negative/positive by -/+ key) and press OK key.
Display/adj/set range | -128 to 127
Unit | 0.1 mm
Default value | 0
LOOP-CST | Registration loop amount adj: casette feeding
Lv.1 | Details | The paper feeding distance is increased/decreased by changing the value. +: The loop amount increases. -: The loop amount decreases.
Use case | When replacing the DC Controller PCB/clearing RAM data When the casette feeding paper is skewed
Adj/set/operate method | Enter the setting value (switch negative/positive by -/+ key) and press OK key.
Display/adj/set range | -128 to 127
Unit | 0.1 mm
LOOP-MF | Registration loop amount adj: manual-feeding
Lv.1 | Details | The paper feeding distance is increased/decreased by changing the value. +: The loop amount increases. -: The loop amount decreases.
Use case | When replacing the DC Controller PCB/clearing RAM data When the manual feeding paper is skewed
Adj/set/operate method | Enter the setting value (switch negative/positive by -/+ key) and press OK key.
Display/adj/set range | -128 to 127
Unit | 0.1 mm
ADJ-REFE | Write start pstn in horz scan: 2nd side

Lv.1

Details

To adjust the image write start position on the second side in the horizontal scanning direction.
The image write start position is set in the relative amount against the first side regardless of the paper pickup cassette/tray/deck.
As the value is incremented by 1, the margin on the left edge of paper is increased by 0.1 mm.
+: Left margin becomes larger. (An image moves to the right.)
-: Left margin becomes smaller. (An image moves to the left.)
When replacing the DC Controller PCB/clearing RAM data, enter the value of service label.

Use case | When replacing the DC Controller PCB/clearing RAM data
Adj/set/operate method | Enter the setting value (switch negative/positive by -/+ key) and press OK key.
Display/adj/set range | -128 to 127
Unit | 0.1 mm
Default value | 0
LOOPREFE | Registration loop amount adj: 2-sided feeding
Lv.1 | Details | The paper feeding distance is increased/decreased by changing the value. +: The loop amount increases. -: The loop amount decreases.
Use case | When replacing the DC Controller PCB/clearing RAM data When the 2-sided paper is skewed
Adj/set/operate method | Enter the setting value (switch negative/positive by -/+ key) and press OK key.
Display/adj/set range | -128 to 127
Unit | 0.1 mm
RG-HF-SP | Regist clutch on timing adj: manual feeding
Lv.1 | Details | The on timing of the registration clutch becomes fast/slow by changing the value. +: The on timing becomes fast. -: The on timing becomes slow. When replacing the DC Controller PCB/clearing RAM data, enter the value of service label.
Use case | When replacing the DC Controller PCB/clearing RAM data
Adj/set/operate method | Enter the setting value (switch negative/positive by -/+ key) and press OK key.
Display/adj/set range | -128 to 127
Unit | 0.1 mm
Default value | 0
ADJ-RE-L | Side regist adj: 2-sided with large paper (more than LTR)

Lv.1

Details

To adjust the image reading start position in horizontal scanning direction for 2-sided print.
As the value is incremented by 0.1, the left blank area changes by 0.1mm.
+: The left blank area becomes narrow. (The image shifts to left)
-: The left blank area becomes wide. (The image shifts to right)
When replacing the DC Controller PCB/clearing RAM data, enter the value of service label.

Use case | When replacing the DC Controller PCB/clearing RAM data
Adj/set/operate method | Enter the setting value (switch negative/positive by -/+ key) and press OK key.
Display/adj/set range | -128 to 127
Unit | 0.1 mm
Default value | -20
LOOP-THK | Registration loop amount adj: thick paper feeding from MP Tray
Lv.1 | Details | The paper feeding distance is increased/decreased by changing the value. +: The loop amount increases. -: The loop amount decreases.
Use case | When replacing the DC Controller PCB/clearing RAM data When the thick paper is skewed
Adj/set/operate method | Enter the setting value (switch negative/positive by -/+ key) and press OK key.
Display/adj/set range | -128 to 127
Unit | 0.1 mm
Default value |
LOOP-SP | Registration loop amount adj: special paper feeding
Lv.1 | Details | The paper feeding distance is increased/decreased by changing the value. +: The loop amount increases. -: The loop amount decreases.
Use case | When replacing the DC Controller PCB/clearing RAM data When the special paper is skewed
Adj/set/operate method | Enter the setting value (switch negative/positive by -/+ key) and press OK key.
Display/adj/set range | -128 to 127
Unit | 0.1 mm
LOOP-ENV | Registration loop amount adj: casette feeding of envelope
Lv.1 | Details | The paper feeding distance is increased/decreased by changing the value. +: The loop amount increases. -: The loop amount decreases.
Use case | When replacing the DC Controller PCB/clearing RAM data When the envelope is skewed at the casette feeding
Adj/set/operate method | Enter the setting value (switch negative/positive by -/+ key) and press OK key.
Display/adj/set range | -128 to 127
Unit | 0.1 mm
ADJ-PTMG | Feed timing Adj
Lv.1 | Details | To adjust the paper feeding timing according to the feed allowance temperature. (regardless of the fixing mode)
Use case | Use to shorten the first copy time or the warm up time.
Adj/set/operate method | Enter the setting value (switch negative/positive by -/+ key) and press OK key.
Display/adj/set range | 0 to 2: +15 degree 3 to 11: each 3 degree 12 to 14: -15degree
Default value | 7