﻿Removing the Toner Supply Assembly

| Print out this category

Removing the Toner Supply Assembly
<Procedure>
1) Remove the inside base cover. (Reference)
2) Remove the left cover. (Reference)
3) Remove the waste toner container. (Reference)
4) Remove the drum unit. (Reference)
5)Remove the toner cartridge.
6) Remove the toner supply cover. (Reference)
7) Remove the delivery tray. (Reference)
8) Remove the developing assembly. (Reference)
9) Remove the laser scanner unit.(Reference)
10) Remove the toner supply assembly.
1 connectors
1 screw
CAUTION:
When removing the toner supply unit, do not incline the toner supply unit not to shed toner.
<Processing after replacing the parts>
NOTE:
The service parts for toner supply unit do not come with a bottle ring. Remove the bottle ring from the old toner supply unit and attach it to the new one.
1) Remove the bottle base.
2 screws
2) Remove the bottle ring.