Checking by the Remote Host Address

| Print out this category

Checking by the Remote Host Address
Using the remote host address to execute Ping can check whether connection to the network is enabled or not.
Remote host address: IP address of PC terminal connected/running on TCP/IP network environment that connects to this equipment.
1) Inform the system administrator about checking of the network connection using Ping.
2) Confirm the remote host address with the system administrator.
3) Enter the remote host address to Ping.
The network is properly connected if the message say "Response from the host".
The network is not properly connected if the message say "No response from the host", therefore, execute the following troubleshooting.