Action to take when replacing parts

| Print out this category

Action to take when replacing parts

Part name | Action
CCD unit | Platen board cover white level automatic adjustment ADF white level adjustment (This action is applicable only when the DADF is installed in the host machine.) The values input of the label included to the new CCD unit
Copyboard glass | White plate data adjustment Platen board cover white level automatic adjustment ADF white level adjustment (This action is applicable only when the DADF is installed in the host machine.)
Stream reading glass | Platen board cover white level automatic adjustment ADF white level adjustment