Disassembling/Assembling and Installing the HDD Removed from the Host Machine

| Print out this category

Disassembling/Assembling and Installing the HDD Removed from the Host Machine
1) Remove the HDD from the HDD Fixation Plate Unit. (The removed HDD Fixation Plate and the screws will not be used.)
2 Screws
2) Remove the HDD from the HDD Support Plate. (The removed HDD and screws will be used in a later step.)
4 Screws
3) Install the HDD Connector Plate first, and then HDD to the HDD Support Plate. (Use the HDD and screws removed in previous step.)
4 Screws
NOTE:
When tightening the screen, be sure to align the screw holes by lifting the HDD Connector Plate and HDD.
CAUTION:
Assembling the option HDD, be careful of the installation direction.
Make sure that the label on the option HDD is facing up.
Install it in the position where the HDD connector is placed in the side with screw hole of HDD Support Plate. (opposite direction compared to the fixed HDD)
4) Install the Conversion Connector.
CAUTION:
Make sure that there is no opening between the Conversion Connector and part of HDD.
5) Fit the 2 bosses of Connector Fixing Block to the hole of Conversion Connector and install it.
2 Screws (P Tight; M3X8)
CAUTION:
Be sure not to tighten the screws in wrong order. Otherwise, the Conversion Connector will not be secured properly.
CAUTION:
Be sure to firmly hold the Connector Fixation Block when tightening the screws.
Be sure to follow the correct order to tighten the screws, otherwise the Conversion Connector may not be connected properly, resulting in poor contact.
6) Install the HDD Cover.
1 Claw
1 Screw (TP Round End; M3X6)
CAUTION:
Be sure to use the round end screw included in the Removable HDD Kit as the TP screw.
7) Install the HDD Handle.
2 Screws (TP Round End; M3X6)
CAUTION:
Be sure to use the round end screw included in the Removable HDD Kit as the TP screw.
8) Affix the HDD No.1 Label to the handle of the Removable HDD.
9) Write down the serial number of the host machine to the label for recording the number, and affix it to the area indicated in the figure.