Assembling the Option HDD

| Print out this category

Assembling the Option HDD
1) Remove the HDD from the HDD Fixation Plate Unit.
2 Screws (The removed screws will not be used.)
2) Remove the 4 Anti-vibration Dampers from the HDD Support Plate. (Use the Anti-vibration Dampers only.)
4 Screws
4 Spacers
HDD
3) Assemble the option HDD.
CAUTION:
Be sure to use the Anti-vibration Dampers removed from the standard HDD.
Never use the parts included in 2.5inch/250GB HDD-D1.
NOTE:
When tightening the screen, be sure to align the screw holes by lifting the HDD.
1 HDD Support Pate (enclosed with option HDD)
4 Anti-vibration Damper (Anti-vibration Damper removed from the standard HDD.)
4 Spacers (enclosed with option HDD)
1 Option HDD (enclosed with option HDD)
4 Screws (binding with flat washer; M3X14) (enclosed with option HDD)
CAUTION:
Assembling the option HDD, be careful of the installation direction.
Make sure that the label on the option HDD is facing up.
Make sure that [A] part of HDD Support Plate is placed at the opposite side of connector.
4) Assemble the second Option HDD.
CAUTION:
Be sure to use the Anti-vibration Damper included in HDD Mirroring Kit-F1 or HDD Data Encryption & Mirroring Kit-C4.
Never use the parts included in 2.5inch/250GB HDD-D1.
NOTE:
When tightening the screen, be sure to align the screw holes by lifting the HDD.
1 HDD Support Pate (enclosed with option HDD)
4 Anti-vibration Damper (enclosed with HDD Mirroring Kit or HDD Data Encryption & Mirroring Kit.)
4 Spacers (enclosed with option HDD)
1 Option HDD (enclosed with option HDD)
4 Screws (binding with flat washer; M3X14) (enclosed with option HDD)
CAUTION:
Assembling the option HDD, be careful of the installation direction.
Make sure that the label on the option HDD is facing up.
Make sure that [A] part of HDD Support Plate is placed at the opposite side of connector.