Requirements for Backup Using the SST

| Print out this category

Requirements for Backup Using the SST
The following conditions must be met for use of the function:
1) Device Firmware Version
Device Firmware Version for SST (Ver4.2x)

| Boot ROM | System | SST
iR-ADV C2030/C2020 series | Boot ROM is not equipped. | Already supported since the 1st version. | The version supporting the corresponding devices.
imageRUNNER ADVANCE series other than iR-ADV C2030/C2020 series | Already supported since the 1st version. | Already supported since the 1st version. | The version supporting the corresponding devices.

2) SST Version
Version 4.2.x or later. An earlier version will not permit the use of the function. If needed, upgrade the SST.
3) Space for backup
To back up the HDDof the iR, the PC must have approx 1024MB of free space at maximum. Sizes of backup files depend on actual data capacities to be backed up.