MISC-P

| Print out this category

MISC-P

COPIER>FUNCTION>MISC-R
P-PRINT | Output of service mode setting value
Lv.1 | Details | To print the service mode setting value.
Use case | Before executing the CLEAR service mode, etc.
Adj/set/operate method | Select the item, and then press OK key.
Required time | Approx. 60 seconds
KEY-HIST | Output of Ctrl Panel key input history
Lv.1 | Details | To print the key input history on the Control Panel.
Use case | When printing the key input history on the Control Panel
Adj/set/operate method | Select the item, and then press OK key.
Required time | Approx. 40 seconds
HIST-PRT | Output of jam and error history
Lv.1 | Details | To print the jam history and error history.
Use case | When printing the jam/error history
Adj/set/operate method | Select the item, and then press OK key.
Required time | Approx. 30 seconds
TRS-DATA | Moving memory reception data to Inbox
Lv.2 | Details | To move the data received in memory to Inbox.
Use case | When moving the data received in memory to Inbox
Adj/set/operate method | Select the item, and then press OK key.
USER-PRT | Output of user mode list
Lv.1 | Details | To print the user mode list.
Use case | When printing the user mode list
Adj/set/operate method | Select the item, and then press OK key.
Required time | Approx. 35 seconds
Supplement/memo | It takes approximately 3 seconds before printing starts.
LBL-PRNT | Output of service label
Lv.1 | Details | To print the service label.
Use case | When printing the service label
Adj/set/operate method | 1) Place A4/LTR paper in Cassette 1. 2) Select the item, and then press OK key.
Required time | Approx. 55 seconds
Supplement/memo | It takes approximately 15 seconds before printing starts.
ENV-PRT | Temp&hmdy/surface temp of Fix Roll log
Lv.1 | Details | To output data of the temperature and humidity inside the machine/surface temperature of the Fixing Roller as a log.
Use case | When figuring out the past temperature inside the machine/fixing temperature information at trouble analysis
Adj/set/operate method | Select the item, and then press OK key.
Required time | Approx. 30 seconds
PJH-P-1 | Detail info of print job history:100 job
Lv.1 | Details | To print the print job history for the latest 100 jobs with detailed information. In the case of less than 100 jobs, the history of all print jobs is printed.
Use case | When printing the print job history with detailed information
Adj/set/operate method | Select the item, and then press OK key.
Supplement/memo | Output the print job history with detailed information which is not displayed/printed in the job history screen under "System Monitor>Print>Log>Printer" and in the report of the print job history.
PJH-P-2 | Detail info of print job history:all job
Lv.1 | Details | To print the history of all print jobs stored in the machine with detailed information (for maximum 5000 jobs). The difference between PJH-P-1 and this item is only the number of jobs printed.
Use case | When printing the print job history with detailed information
Adj/set/operate method | Select the item, and then press OK key.
Supplement/memo | Output the print job history with detailed information which is not displayed/printed in the job history screen under "System Monitor>Print>Log>Printer" and in the report of the print job history.
USBH-PRT | Output of USB device information report
Lv.1 | Details | To output information of the connected USB device in the form of a report.
Adj/set/operate method | Select the item, and then press OK key.