﻿Removing the Toner Supply Cover

| Print out this category

Removing the Toner Supply Cover
1) Open the front cover.
2) Open the right cover.
3) Turn the lock lever as shown to release the lock of the waste toner container.
4) Remove the waste toner container.
5) Remove the screw securing the developing assembly pressure lever.
6) Turn the lever in the direction of the arrow to release the drum unit lock.
7) Remove the drum unit.
8) Open the toner supply cover.
9) Remove the toner container.
10) Remove the 2 Screws.
11) Remove the link cover.
1 Claw
12) Disengage the Link Lever from the shaft.
13) Remove the toner supply cover.
1 Claw
NOTE:
When closing the toner cover without the toner container, push the lock release lever.