Installing the Reader Heater

| Print out this category

Installing the Reader Heater
1) Open the ADF (or platen Cover).
2) Detach the glass retainer (right).
2 Screws
3) Remove the platen glass.
4) Move the drive belt in the arrow direction to shift the CCD unit to the center.
5) Attach the 2 supplied wire saddles (small).
6) Attach the heater on the left of the reader.
1 Connector
1 Screw
2 Clamps
7) Attach the 1 supplied wire saddle (small).
8) Joint the 1 connector.
9) Attach the heater on the left of the right.
1 Screw
1 Clamp
10) Restore the following parts:
Platen glass
Glass retainer (right) (2 Stepped Screws)
Lower rear cover (4 Screws)
Connector (When the cassette pedestal is installed.)
Connector cover (1 Screw)
Left rear cover (4 Screws)
Rear cover (4 Screws)(Tighten the screws in the following order: upper left, lower left, upper right, and then lower right.)
Power cord clamp (1 Screw) (100/120V model only)
Power cord
11) Turn the enviorment heater switch ON.