Flying start temperature control

| Print out this category

Flying start temperature control
Purpose:
To reduce the print time (FPOT) of the 1st sheet
Starting conditions
• When opening the copyboard cover or ADF, and also the detection temperature of the main thermistor is less than 100 deg C.
• When the original sheet is set on the ADF tray, and also the detection temperature of the main thermistor is less than 100 deg C.
• When the main power switch is turned ON or the machine condition is shift from the sleep mode to standby, and also the detection temperature of the main thermistor is less than 180 deg C.
Control description:
• The target control temperature is set to 155 deg C and the fixing motor starts to rotate with a half speed. The control continues for maximum 10 seconds.