Points to Make Before Installation

| Print out this category

Points to Make Before Installation
Be sure to go through the following before starting the work.
1) Imaging faults can result due to dew condensation that occurs when the machine is moved from a cold place to a warm place. Leave the unpacked machine as it is for at least two hours before installing it.
(Dew condensation: When a metallic object is brought from a low-temperature place to a high-temperature place, water vapor around it is cooled abruptly and consequently water drops stick to the surface of the metallic object.)
2) The maximum weight of the machine is approx. 78.9 kg ( FAX standard model). Be sure to perform the work in accordance with the standard to handle a heavy load in each country. In addition, be sure to keep the machine leveled when lifting it.
3) This product was designed considering the potential connection to the Norwegian IT power distribution system