Steps to E-RDS settings﻿

| Print out this category

Steps to E-RDS settings﻿
1. Start [Service Mode] at Level 1.
1) Press [Settings/Registration (User Mode)] button on the control panel.
2) Press [2] and [8] buttons at a time on the control panel.
3) Press [Settings/Registration (User Mode)] button on the control panel.
4) [Service Mode] screen is shown. Touch the [Mode List] button or the [Mode List Classic] button.
2. Select [COPIER] > [Function] > [CLEAR] > [ERDS-DAT] and touch the [OK] button.
NOTE:
This operation initializes the E-RDS settings to factory setting values.
For the setting values to be initialized, see the section of “Initializing E-RDS settings”.
3. Perform installation or deletion of the CA certificate if necessary, and reboot the device.
Installation of the CA certificate: Perform installation from SST.
Deletion of the CA certificate: When the following operation is performed, the CA certificate in the factory setting is automatically installed.
(1) Start [Service Mode] at Level 2.
1) Press [Settings/Registration (User Mode)] button on the control panel.
2) Press [2] and [8] buttons at a time on the control panel.
3) Press [Settings/Registration (User Mode)] button on the control panel.
4) Touch the [Mode List] button or the [Mode List Classic] button on the [Service Mode] screen.
5) Press [Settings/Registration (User Mode)] button on the control panel.
6) Press [2] button on the control panel.
(2) Select [COPIER] > [Function] > [CLEAR] > [CA-KEY] and touch the [OK] button.
“OK!” is displayed if the CA certificate is initialized. When “NG!” is displayed, see the section of “Troubleshooting” to execute the remedy, and then perform initialization of the CA certificate again and check to see if the CA certificate is initialized.
(3) Reboot the device.
4. Activate [SERVICE MODE] in LEVEL 1. (See 1. for the procedure.)
5. Select [COPIER] > [Function] > [INSTALL] > [E-RDS].
6. Touch the numeric button [1] on the control panel (the setting value is changed to 1) and touch the [OK] button. (The data is reflected to the setting value field.)
NOTE:
This operation enables the communication function with UGW.
CAUTION:
The following settings i.e. RGW-PORT and RGW-ADR in Service mode must not be change unless there are specific instructions to do so.
Changing these values will cause error in communication with UGW.
7. Select [COM-TEST] and then touch [OK].
NOTE:
This initiates the communication test between the device and the UGW.
If the communication is successful, “OK!” is displayed. If “NG!” (failed) appears, refer to the “Troubleshooting“ and repeat until “OK!” is displayed.
NOTE:
The communication results with UGW can be distinguished by referring to the COM-LOG. By performing the communication test with UGW, E-RDS acquires schedule information and starts monitoring and meter reads operation.