Assembling and Installing the Option HDD (Second HDD)

| Print out this category

Assembling and Installing the Option HDD (Second HDD)
1) Assemble the option HDD.
CAUTION:
Be sure to use the Anti-vibration Damper included in HDD Mirroring Kit-F1 or HDD Data Encryption & Mirroring Kit-C4.
Never use the parts included in 2.5inch/250GB HDD-D1.
NOTE:
When tightening the screen, be sure to align the screw holes by lifting the HDD Connector Plate and HDD.
1 HDD Support Plate (enclosed with option HDD)
4 Anti-vibration Damper (enclosed with HDD Mirroring Kit or HDD Data Encryption & Mirroring Kit.)
1 HDD Connector Plate (enclosed with removable HDD Kit)
1 Option HDD (enclosed with option HDD)
4 Spacers (enclosed with option HDD)
4 Screws (binding with flat washer; M3X14) (enclosed with option HDD)
CAUTION:
Assembling the option HDD, be careful of the installation direction.
Make sure that the label on the option HDD is facing up.
Install it in the position where the HDD connector is placed in the side with screw hole of HDD Support Plate. (opposite direction compared to the fixed HDD)
2) Install the Conversion Connector.
CAUTION:
Make sure that there is no opening between the Conversion Connector and part of HDD.
3) Fit the 2 bosses of Connector Fixing Block to the hole of Conversion Connector and install it.
2 Screws (P Tight; M3X8)
CAUTION:
Be sure not to tighten the screws in wrong order. Otherwise, the Conversion Connector will not be secured properly.
CAUTION:
Be sure to firmly hold the Connector Fixation Block when tightening the screws.
Be sure to follow the correct order to tighten the screws, otherwise the Conversion Connector may not be connected properly, resulting in poor contact.
4) Install the HDD Cover.
1 Claw
1 Screw (TP Round End; M3X6)
CAUTION:
Be sure to use the round end screw included in the Removable HDD Kit as the TP screw.
5) Install the HDD Handle.
2 Screws (TP Round End; M3X6)
CAUTION:
Be sure to use the round end screw included in the Removable HDD Kit as the TP screw.
6) Affix the HDD No.2 Label to the handle of the Removable HDD.
7) Write down the serial number of the host machine to the label for recording the number, and affix it to the area indicated in the figure.