Pickup position code

| Print out this category

Pickup position code
When jam occurs, pickup location is indicated with the following pickup position code.

Pickup position | Pickup position code
At Finisher jam/At error avoidance jam/At ADF jam without pickup operation (at SEND, Inbox, etc.) | 00
Cassette 1 | 01
Cassette 2 | 02
Multi-purpose Tray | 05
Side Paper Deck | 06
Duplex (At duplex printing, jam occurs after paper passes through the Duplex Feed Sensor (S7).) | F0