Protection features

| Print out this category

Protection features

Code | Description | Error Clear
E000 | Fixing temperature abnormal rise
0001 | The temperature detected by the main thermistor does not rise to the specified value during startup control. | Yes
E001 | Fixing unit temperature rise detection
0000 | The reading of the main thermistor is 250 deg C or more continuously for 200 msec. | Yes
0001 | The hardware circuit detects overheating of the main or sub thermistor for 200 msec. | Yes
0002 | The reading of the sub thermistor is 295 deg C or more continuously for 200 msec. | Yes
E002 | Fixing unit temperature insufficient rise
0000 | 1.The reading of the main thermistor is less than 115 deg C continuously for 400 msec 1.3 sec after it has indicated 100 deg C. 2.The reading of the main thermistor is less than 150 deg C continuously for 400 msec 1.3 sec after it has indicated 140 deg C. | Yes
E003 | Low fixing temperature detection after standby
0000 | The reading of the main thermistor is less than 140 deg C continuously for 400 msec or more. | Yes
E004 | Thermistor disconnection detection error
0000 | When disconnection is detected with connector (J214) for 30 sec continuously. | No
E014 | Unstable rotation of the Fixing Motor (M2)
0001 | Detection is executed every 100 msec after the start of motor rotation; however, the drive detection signal is absent for 2 sec. |
0002 | During motor rotation, detection is executed every 100 msec; however, the drive signal is absent 5 times in sequence. | No
E261 | Error in Zero Cross
0000 | Zero Cross failed to be detected for 500ms or more while the relay was ON. * The same condition is detected after the error retry is performed. | No

Related Service Mode
• Error code clear
COPIER > FUNCTION > CLEAR > ERR