USER

| Print out this category

USER

COPIER>OPTION>USER
COPY-LIM | Setting of upper limit for copy
Lv.1 | Details | To set the upper limit value for copy.
Use case | Upon user's request
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 1 to 9999
Default value | 999
SLEEP | Setting of auto sleep function
Lv.1 | Details | To set ON/OFF of auto sleep function.
Use case | Upon user's request
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 0 to 1 0: OFF, 1: ON
Default value | 1
SIZE-DET | ON/OFF of original size detect function
Lv.1 | Details | To set ON/OFF of original size detection function.
Use case | Upon user's request (glare of the scan lamp, etc)
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 0 to 1 0: OFF, 1: ON
Default value | 1
COUNTER1 | Display of software counter 1
Lv.1 | Details | To display counter type for software counter 1 on the Counter Check screen.
Use case | Upon user/dealer's request
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Caution | Display only. No change is available.
Default value | The value differs according to the location.
COUNTER2 | Setting of software counter 2
Lv.1 | Details | To set counter type for software counter 2 on the Counter Check screen.
Use case | Upon user/dealer's request
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 0 to 999
Default value | The value differs according to the location.
COUNTER3 | Setting of software counter 3
Lv.1 | Details | To set counter type for software counter 3 on the Counter Check screen.
Use case | Upon user/dealer's request
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 0 to 999
Default value | The value differs according to the location.
COUNTER4 | Setting of software counter 4
Lv.1 | Details | To set counter type for software counter 4 on the Counter Check screen.
Use case | Upon user/dealer's request
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 0 to 999
Default value | The value differs according to the location.
COUNTER5 | Setting of software counter 5
Lv.1 | Details | To set counter type for software counter 5 on the Counter Check screen.
Use case | Upon user/dealer's request
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 0 to 999
Default value | 0
COUNTER6 | Setting of software counter 6
Lv.1 | Details | To set counter type for software counter 6 on the Counter Check screen.
Use case | Upon user/dealer's request
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 0 to 999
Default value | 0
DATE-DSP | Setting of data/time display format
Lv.1 | Details | To set date/time display format according to the country or region. After the display format is set with this mode, the order of date is reflected to the followings: Preferences > Timer/Energy Settings > Date/Time Settings, and report output.
Use case | Upon user's request
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 0 to 2 0: YYMM/DD, 1: DD/MMYY, 2: MM/DD/YY
Default value | The value differs according to the location.
Related user mode | Preferences > Timer/Energy Settings > Date/Time Settings
MB-CCV | Control card usage limit for Mail Box
Lv.1 | Details | To restrict use of control card for Mail Box.
Use case | Upon user's request
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 0 to 1 0: Unlimited, 1: Limited
Default value | 1
CONTROL | Charge setting of PDL job
Lv.1 | Details | To set charge count transmission of PDL job to the connecting charging management device (Coin Manager or non-Canon-made control card).
Use case | Upon user's request
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 0 to 1 0: No charge, 1: Charge
Default value | 0
B4-L-CNT | Count setting of B4 size
Lv.1 | Details | To set B4 count with software counter 1 to 8 as to whether B4 is counted as large size or small size. Selecting 1 counts B4 or larger size paper as large size while paper smaller than B4 size as small size.
Use case | Upon user's request
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 0 to 1 0: Small size, 1: Large size
Default value | 0
Related service mode | COPIER> OPTION> FNC-SW> SC-L-CNT
TRY-STP | Set of Fin Tray output suspension ref
Lv.1 | Details | To set the reference which judges to suspend outputting to Finisher Tray.
Use case | Upon user's request
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 0 to 1 0: At detection of full tray, 1: At detection of height
Default value | 0
MF-LG-ST | Dis/hide of long strip mode
Lv.1 | Details | To set whether to display or hide the [Long Original] button. When 1 is set, [Long Original] button is displayed in Copy > Options screen and the long strip paper becomes available.
Use case | Upon user's request (use of long strip original or long strip paper)
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 0 to 1 0: Hide, 1: Display
Default value | 0
Related user mode | Copy > Options
Supplement/memo | Up to 630mm length paper is supported when DADF is used.
CNT-DISP | Display/hide of serial No.
Lv.1 | Details | To set whether to display or hide the serial No. on the Counter Check screen.
Use case | When setting to display/hide serial No. on the Counter Check screen.
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 0 to 1 0: Display, 1: Hide
Default value | 0
PH-D-SEL | Set dither matrix at screen processing
Lv.1 | Details | To set the screen dither matrix to be used for half toning processing at the time of copy output, B&W Inbox scan output and B&W SEND output. When moire occurs frequently, set to ""1: 141 lines"". When the setting is changed, the number of PG lines to be output at PASCAL control is also changed.
Use case | When moire frequently occurs at the time of copy output, B&W Inbox scan output and B&W SEND output. Especially when moire frequently occurs in the halftone density area of photo and image gradation areas
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 0 to 1 0: 134 lines, 1: 141 lines
Default value | 1
Related service mode | COPIER> OPTION> USER> PH-D-SL2
COPY-JOB |  | Setting of copy job reservation
Lv.1 | Details | To set to enable/disable copy job reservation when the Card Reader/Coin Manager is used.
Use case | Upon user's request
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 0 to 1 0: Enabled, 1: Disabled
Default value | 0
OP-SZ-DT | Orgnl size dtct ON/OFF at copyboard open
Lv.1 | Details | To set ON/OFF of original size detection while the Copyboard is opened. When ""0: OFF"" is set, enter original size manually from the Control Panel. When ""1: ON"" is set, original size is detected automatically.
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 0 to 1 0: OFF, 1: ON
Default value | 0
NW-SCAN | Setting of network scan function usage
Lv.1 | Details | To set to enable/disable use of network scan function.
Use case | Upon user's request
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Caution | - Do not change this mode in Japan. - For PS/PCL machines for overseas (outside Japan), fix the setting value as ""1: Enabled"". For others, permit the use.
Display/adj/set range | 0 to 1 0: Disabled, 1: Enabled
HDCR-DSP | Setting of HDD complete delete method
Lv.1 | Details | To set data deletion method of HDD data complete deletion function.
Use case | When switching the deletion method in HDD data complete deletion mode
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 1 to 4 1: 1-time deletion with 0 data, 2: 1-time deletion with random data, 3: 3-time deletion with random data, 4: DOD
Default value | 1
Supplement/memo | HDD data complete deletion function: a function to completely delete data in HDD by overwriting with 0 (null) data or random data to the file data when logically deleting file on HDD (deleting management information data).
JOB-INVL | Job intvl setting at interruption copy
Lv.1 | Details | To set output interval between jobs at the time of interruption copy. Sorting is difficult after interruption copy because of the continuous output of the next job. Paper interval becomes longer when starting pickup for the next job after the last sheet of the previous job is delivered.
Use case | Upon user's request
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 0 to 2 0: Continuous output of the interruption copy and the next job 1: Starting pickup for the next job after the interruption copy is delivered all. 2: Starting pickup for the next job after the previous job is delivered all. (For all jobs)
Default value | 0
TAB-ROT | [Not used]
PR-PSESW | Display/hide of output Stop button
Lv.1 | Details | To set whether to display or hide [Stop] button on the Status Monitor screen.
Use case | - Upon user's request - When promptly stopping the print job in operation or under reservation
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 0 to 1 0: Hide, 1: Display
Default value | 0
IDPRN-SW | Charge target job set of dept mngm cntr
Lv.1 | Details | To set the job type that advances the department management counter.
Use case | Upon user's request
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.

Display/adj/set range

0 to 1
0:
PRINT category: Inbox Print, Report Print, Send Local Print, PDL Print
COPY category: COPY
1:
PRINT category: Report Print, Send Local Print, PDL Print
COPY category: COPY, Inbox Print

Default value | 0
PCL-COPY | Set of PCL COPIES command control method
Lv.1 | Details | To set the binder control method of COPIES command with PCL. Select whether to use the control method of Canon-made PCL or use the same control method of non-Canon-made PCL.
Use case | Upon user's request
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.

Display/adj/set range

0 to 65535
0: Control method of Canon-made PCL (following the value of COPIES command that is specified for each page to control on a page basis)
1: Control method of non-Canon-made PCL (handling the value of COPIES command, which is specified for page 1 at the time of Collate mode, as bind figure while the value of COPIES command for the next page or later is invalid. Same control applies as Canon-made PCL at the time of non-sorted mode)
2 to 65535: For future use

Default value | 0
CNT-SW | Set default dis items on charge counter
Lv.1 | Details | To set default display items of the charge counter on the Counter Check screen.
Use case | Upon user's request
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Caution | Do not use this mode overseas (outside Japan).

Display/adj/set range

0 to 2
For Japan
0: Counter 1 - Total 1: 101
1: Counter 1 - Total 2: 102, Counter 2 - Copy (Total 2): 202, Counter 3 - Total A2: 127
2: Not used
For UL
0: Counter 1 - Total 1: 101, Counter 2 - Total (Large): 103, Counter 3 - Copy (Total 1): 201, Counter 4 - Copy (Large): 203
1: Counter 1 - Total 2: 102, Counter 2 - Copy (Total 2): 202
2: Not used

Default value | 0
BCNT-AST | Set of box print charge target job
Lv.1 | Details | To set the job type that advances the count in box print with NE Controller (ASSIST).
Use case | When switching the job type that is subject to counting of the box print with NE Controller
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 0 to 1 0: PDL job, 1: Copy job
Default value | 0
PRJOB-CP | Set count TX at RX/report print
Lv.1 | Details | To set to enable/disable a page-basis count pulse transmission to the charging management device at the time of reception print or report print.
Use case | Upon user's request
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 0 to 1 0: No transmission, 1: Transmission
Default value | 0
Supplement/memo | Charging management device: Coin Manager, Non-Canon-made control card
DOC-REM | Dis/hide of original removal message
Lv.1 | Details | To set whether to display or hide the message to remove original when scanning with DADF without opening/closing DADF after scanning with the Copyboard.
Use case | Upon user's request
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 0 to 1 0: Hide, 1: Display
Default value | 0
DPT-ID-7 | Password entry set at dept ID reg/auth
Lv.1 | Details | To set whether to require a password entry at the time of registration/authentication of department ID. With the setting to require entry, entry of 7-digit password is required as well as entry of department ID.
Use case | Upon user's request
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 0 to 1 0: Department ID only, 1: 7-digit (password) entry
Default value | 0
RUI-RJT | Connct set at invalid auth from remoteUI
Lv.1 | Details | To set to disconnect HTTP port when the machine receives invalid authentication from remote UI 3 times.
Use case | Upon user's request
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 0 to 1 0: Continued connection, 1: Disconnected
Default value | 0
FREG-SW | Dis/hide of MEAP counter free rgst area
Lv.1 | Details | To set whether to display or hide the free register area of MEAP counter for SEND
Use case | At trouble analysis
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Caution | - Do not use this at the normal service. - Take necessary action in accordance with the instructions from the Quality Support Division.
Display/adj/set range | 0 to 1 0: Hide, 1: Display
Default value | 0
Supplement/memo | Individual count-up (counter advance) of MEAP application is available in the free register area of MEAP counter.
IFAX-SZL | Setting of IFAX send size limit
Lv.1 | Details | To set for restricting data size at the time of IFAX transmission that does not go through the server. With the setting to restrict the data size, there will be #830 error in the case of sending data that exceeds the upper limit value. In the case that the data goes through the server, the size of transmission data is always restricted.
Use case | Upon user's request
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 0 to 1 0: Limited, 1: Not limited (Restriction applies when data goes through the server.)
Default value | 1
Related user mode | Function Settings > Send > E-Mail/I-Fax Settings > Maximum Data Size for Sending
Supplement/memo | Specify the upper limit value for transmission data size in user mode.
IFAX-PGD | Set page split TX at IFAX Simple mode TX
Lv.1 | Details | To set to enable/disable split-data transmission on a page basis in the case that the transmission size in IFAX Simple mode exceeds the upper limit value.
Use case | Upon user's request
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Caution | In the case to enable split-data transmission, be sure to get approval from the user by explaining the following: - No guarantee for page order on the reception side - There is a possibility of interruption of other received jobs between pages.
Display/adj/set range | 0 to 1 0: Disabled, 1: Enabled
Default value | 0
Related service mode | COPIER> OPTION> CLEANING> W-CLN-P
Related user mode | Function Settings > Send > E-Mail/I-Fax Settings > Maximum Data Size for Sending
Supplement/memo | Specify the upper limit value for transmission data size in user mode.
MEAPSAFE | Setting of MEAP safe mode
Lv.1 | Details | To set safe mode for MEAP platform. MPSF is displayed on the Control Panel in safe mode. In safe mode, MEAP application is stopped while just the system application, which starts with initial state, is activated. This mode enables obtaining log for cause analysis of MEAP failure.
Use case | Perform system recovery processing when MEAP platform fails to be activated due to resource confliction between MEAP applications, service registration or use order.
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 0 to 1 0: Normal mode, 1: Safe mode
Default value | 0
AFN-PSWD | Access limit setting to user mode
Lv.1 | Details | To set to restrict password entry when accessing to the user mode. With the setting to enable this mode, password entry of system administrator is required after pressing Settings/Registration key.
Use case | Upon user's request
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 0 to 1 0: Password is not required, 1: Password is required
Default value | 0
PTJAM-RC | Auto reprint setting at PDL print jam
Lv.1 | Details | To set to automatically restart printing after jam recovery that occurs with PDL print.
Use case | Upon user's request
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 0 to 1 0: Not automatically reprinted, 1: Automatically reprinted
PDL-NCSW | Card mngm setting for PDL print job
Lv.1 | Details | To set to make PDL print job to be subject to card management by the Card Reader. With the setting to enable this mode, PDL print is available only when the card ID of the card inserted to the Card Reader matches the department ID.
Use case | Upon user's request
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 0 to 1 0: PDL print is available with no card inserted. 1: PDL print is available only when the card ID matches the department ID in the case that the card is inserted.
Default value | 0
SLP-SLCT | Usage setting of network applications
Lv.1 | Details | With the setting to use network-related application, the machine can be recovered through network because it does not move to sleep mode 1. For this machine to recover from sleep mode 1 through network, a particular packet needs to be received; however, the existing network-related application does not send this packet. With the setting not to use the network-related application, this machine cannot recover from sleep mode 1 through network when it gets into sleep mode 1.
Use case | Upon user's request
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Caution | Do not use this at the normal service.
Display/adj/set range | 0 to 1 0: Not used (Shift to sleep mode 1 is available.) 1: Used (Shift to sleep mode 1 is not available.)
Default value | 0
Supplement/memo | Network-related application: NetSpot Accountant, imageWARE
PS-MODE | Compatible mode setting at PS usage
Lv.1 | Details | To set for compatibility with existing machine regarding image process or print specification with PS print. Selecting 1 enables to have the print result equivalent to that of iR2200/2800/3300 series while selecting 2 enables to have the print result equivalent to that of iR105 series.
Use case | At replacement
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.

Display/adj/set range

0 to 65535
0: No use of compatibility mode with PS
1: Image processing equivalent to that of iR2200/2800/3300 series (compatibility with existing machine)
2: Image processing equivalent to that of iR105 (compatibility with existing machine)
3: Spare
4: 2-sided print with landscape and portrait mixed when using Canon-made Controller (compatibility with non-Canon-made Controller)
5 to 65535: Spare

Default value | 0
CNCT-RLZ | Setting of connection serialize function
Lv.1 | Details | Connection serialize is a function to assure job grouping function of imageWARE Output Manager Select Edition V1.0. The setting to enable this mode can avoid job rearrangement because the machine does not receive job data from other connection until it completes job data reception from the current connection.
Use case | Upon user's request
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 0 to 1 0: OFF, 1: ON
Default value | 0
Supplement/memo | Connection: Connection to be established through network between multiple hosts (PC, etc). Job grouping function: A function of imageWARE Output Manager Select Edition V1.0. This is to prevent job interruption from other PC by group job (sending multiple jobs in 1 session at job transmission).
JA-FUNC | ON/OFF of job archive function
Lv.1 | Details | To set ON/OFF of job archive function.
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Caution | Changing this mode is not available in service mode, but reference is available (in service mode). This mode is available only with the MEAP program that supports job archive.
Display/adj/set range | 0 to 1 0: OFF, 1: ON
Default value | 0
JA-JOB | Setting of job archive target job
Lv.1 | Details | To set the job type subject to job archive. With the job archive function enabled, archive operation is executed when executing the target job.
Use case |
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Caution | Changing this mode is not available in service mode, but reference is available (in service mode). This mode is available only with the MEAP program that supports job archive.
Display/adj/set range | 0: N/A, 3: Limited to FAX/IFAX, 0xFFFFFFFF: All jobs
Default value | 0
Related service mode | COPIER > OPTION > USER > JA-FUNC
LDAP-SW | Retrieval condition set for LDAP server
Lv.1 | Details | To set the condition to search e-mail address, etc. from LDAP server.
Use case | When specifying condition to search e-mail address, etc. from LDAP server
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 0 to 5 0: Includes the next, 1: Not include the next, 2: Equivalent to the next, 3: Not equivalent to the next, 4: Starts with the next, 5: Finishes with the next
Default value | 4
Supplement/memo | LDAP (Lightweight Directory Access Protocol): Registering LDAP server enables to search e-mail address, etc. from LDAP server and the result can be registered in the Address Book, etc. Registration is available by the following: Set Destination > Register LDAP Server
FROM-OF | Deletion of mail sender's address
Lv.1 | Details | To set whether to delete the sender's address (From) at the time of e-mail transmission.
Use case | Upon user's request
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 0 to 1 0: Retained, 1: Deleted
Default value | 0
DOM-ADD | Additional entry of mail destn domain
Lv.1 | Details | To set to automatically add the domain specified in user mode to the sending address (To) entered at the time of e-mail transmission. If specifying ""xxx.com"" as a domain in user mode in advance, just entering ""aura"" enables to display ""aaa@xxx.com"" when sending e-mail.
Use case | Upon user's request
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 0 to 1 0: Not added, 1: Added
Default value | 0
FILE-OF | File send prohibition to entered address
Lv.1 | Details | To set to prohibit address entry at the time of file transmission. File transmission is not available by entering the address because of no display of ""File"" on the transmission screen. The addresses already registered in the Address Book can be used.
Use case | Upon user's request
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Caution | To restrict addresses for transmission, be sure to manually delete them because the addresses registered in the Address Book can be used.
Display/adj/set range | 0 to 1 0: Enabled, 1: Disabled
Default value | 0
MAIL-OF | Mail send prohibition to entered address
Lv.1 | Details | To set to prohibit address entry at the time of e-mail transmission. E-mail transmission is not available by entering the address because of no display of ""E-Mail"" on the transmission screen. The addresses already registered in the Address Book can be used.
Use case | Upon user's request
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Caution | To restrict addresses for transmission, be sure to manually delete them because the addresses registered in the Address Book can be used.
Display/adj/set range | 0 to 1 0: Enabled, 1: Disabled
Default value | 0
IFAX-OF | IFAX send prohibition to entered address
Lv.1 | Details | To set to prohibit address entry at the time of I-Fax transmission. IFAX transmission is not available by entering the address because of no display of ""I-Fax"" on the transmission screen. The addresses already registered in the Address Book can be used.
Use case | Upon user's request
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Caution | To restrict addresses for transmission, be sure to manually delete them because the addresses registered in the Address Book can be used.
Display/adj/set range | 0 to 1 0: Enabled, 1: Disabled
Default value | 0
LDAP-DEF | Initial condone set of LDAP server search
Lv.1 | Details | To set initial condition for search target attribute that is specified at the time of LDAP server Details search.
Use case | Upon user's request
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 0 to 6 0: Name, 1: E-mail, 2: FAX, 3: Organization, 4: Organization unit, 5: No registration 1 (any setting), 6: No registration 2 (any setting)
Default value | 0
Related service mode | COPIER > OPTION > USER > LDAP-SW
FREE-DSP | Display/hide of charge disable screen

Lv.1

Details

To set whether to display or hide the Use Charge Management screen for switching between charge and no charge.
The hardware switch for switching charge/no charge in the Coin Manager enables the mode in which all the services are available for free (store manager mode) by temporarily releasing the charging system.
Even without the hardware switch, the mode can be switched with the software switch when it is set to display the Use Charge Management screen in Settings/Registration.

Use case | When enabling all the services to be provided for free by temporarily releasing the charging system
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 0 to 1 0: Hide, 1: Display
Default value | 0
Related user mode | Management Settings > Charge Management > Use Charge Management
CLR-TIM | Set of HDD Entry Kit data delete timing

Lv.1

Details

To set the timing to completely delete the data when HDD Encryption Kit is used.
Selecting 0 may reduce the job processing speed because page data that has been already processed is deleted while the other job is in process, causing overload to CPU and HDD access.
Selecting 1 improves the job processing speed because the process is executed after a job is completed.

Use case | Upon request to improve the job processing speed
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 0 to 1 0: During job process, 1: After the job is completed
Default value | 0
HDCR-DSW | Dis/hide of HDD complete delete ON/OFF
Lv.1 | Details | To set whether to display or hide ""Hard Disk Data Complete Deletion"" in user mode. With this setting, HDD data complete deletion function is available with ON/OFF button on the screen.
Use case | Upon user's request
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 0 to 1 0: Hide, 1: Display
Default value | 0
Related user mode | Management Settings > Data Management > HDD Data Complete Deletion > Hard Disk Data Complete Deletion
Supplement/memo |
SNMP-COA | Inside comity name SNMPaccess limit:admin

Lv.1

Details

To restrict SNMP access by the community name (administrator right) that is kept internally.
This machine internally retains the community name (administrator right) other than the SNMP community name that is specified in user mode. Canon-made utility software, such as NetSpot, uses this community name.
Because of security concern, select 0/1 in the case to restrict SNMP access with the internal community name.

Use case | When restricting SNTP access with the community name (administrator right) that is retained internally
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 0 to 2 0: OFF, 1: Read only, 2: Read/Write
Default value | 2
Related user mode | Preferences > Network > SNMP Settings > Community Name 1 Settings
SCALL-CMP | Set of repair request complete notice
Lv.1 | Details | With this setting enabled, a notification of repair completion is sent to UGW server to clear the repair-request
Use case | Service technician uses this mode after completing repair.
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 0 to 1
Default value | 0
USBH-DSP | Display/hide of "Use USB Host"
Lv.1 | Details | To set whether to display "Preferences > External Interface > USB Settings > Use USB Host". By selecting "1: Display", whether to use USB host on USB Settings screen can be selected.
Use case | When switching to display or hide "Use USB Host" on USB Settings screen
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 0 to 1 0: Hide, 1: Display
Default value | 0
Related user mode | Preferences > External Interface > USB Settings > Use USB Host
USBM-DSP | Dis/hide of USB ex-memory device driver
Lv.1 | Details | To set whether to display "Preferences > External Interface > USB Settings > Use MEAP Driver for USB External Device". By selecting "0: Hide", the item is not displayed, and the user administrator cannot change the setting of the MEAP driver for the USB external memory device.
Use case | When prohibiting the user administrator to change the setting of "Use MEAP Driver for USB External Device", set 0 after the specified setting is completed.
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 0 to 1 0: Hide, 1: Display
Default value | 1
Related user mode | Preferences > External Interface > USB Settings > Use MEAP Driver for USB Input Device
USBI-DSP | Dis/hide of USB input device driver set
Lv.1 | Details | To set whether to display "Preferences > External Interface > USB Settings > Use MEAP Driver for USB Input Device". By selecting "0: Hide", the item is not displayed, and the user administrator cannot change the setting of the MEAP driver for the USB input device.
Use case | When prohibiting the user administrator to change the setting of "Use MEAP Driver for USB Input Device", set 0 after the specified setting is completed.
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 0 to 1 0: Hide, 1: Display
Default value | 1
Related user mode | Preferences > External Interface > USB Settings > Use MEAP Driver for USB Input Device
CTCHKDSP | Display/hide of counter print
Lv.1 | Details | To set whether to display or hide ""Print List"" on the Counter Check screen. Model name, model number information, counter check date and counter information can be output as a total count management report.
Use case | Upon user's request
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 0 to 1 0: Hide, 1: Display
Default value | 1
DFLT-ADJ | Tgt Auto Adj Gradation initial dis set
Lv.1 | Details | To set whether to display "automatic gradation correction" on User mode.
Use case | Upon user's request
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 0 to 3 0: Hide, 1: Display, 2 to 3: Not used
Default value | 0
Related user mode | Settings/Registration> Adjustment/Maintenance> Auto Adjust Gradation
USBR-DSP | Dis/hide of USB infrared device driver
Lv.1 | Details | To set whether to display "Preferences > External Interface > USB Settings > Use MEAP Driver for USB Infrared Device."
Use case | When prohibiting the user administrator to change the setting of "Use MEAP Driver for USB Infrared Device," set 0 after the specified setting is completed.
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 0 to 1 0: Hide, 1: Display
Default value | 0
Related user mode | Preferences > External Interface > USB Settings > Use MEAP Driver for USB Infrared Device
POL-SCAN | Dis/hide of Rights Management Server set
Lv.1 | Details | When ""1: Display"" is set, the Rights Management Server function screen is displayed. While the Rights Management Server function is a standard feature, it is possible to hide if not necessary.
Use case | Upon user's request
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 0 to 1 0: Hide, 1: Display
Default value | 1 (Japan), 0 (Others)
PH-D-SL2 | Set halftone process in text/photo mode

Lv.1

Details

When copying or B&W scanning to Inbox in text/photo mode, halftone processing of the image which reproduces gradation of text and photo judgment areas can be specified with this setting.
Set to 1 when jaggy occurs or request to use the same half toning method (text area) as conventional one is raised.
Set to 2 when moire occurs frequently or request to use the same half toning method as conventional B&W MFP method is raised.
Even 0 is set, TBIC is used for text judgment area and low screen ruling for photo judgment area at the time of B&W Inbox scan.
The setting is disabled when the B&W Inbox scanning density is set to auto.

Use case

- When jaggy occurs on the edge of text or thin lines at copy output. Especially when jaggy occurs in the text or thin lines (text in halftone dots) of the area where gradation in the halftone density is expressed like photo, graphics, etc.
- When moire occurs frequently at the time of copy or B&W Inbox scan Especially when moire frequently occurs in the area where gradation in the halftone density is expressed like photo, graphics, etc. and this symptom is not alleviated with PH-D-SEL or sharpness adjustment
- When receiving a request to use the same half toning method (text area) as the conventional one (model with image area separation method) at copy output
- When receiving a request to use the same half toning method (both text and photo areas) as the conventional B&W MFP method at the time of copy or B&W Inbox output

Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 0 to 2 0: Low screen ruling (134 lines) is used for photo judgment area and high screen ruling (141 lines) for text judgment area. 1: Low screen ruling is used for photo judgment area and TBIC for text judgment area. 2: TBIC is used for both photo and text judgment areas.
Default value | 0
Related service mode | COPIER> OPTION> USER> PH-D-SEL
W-TN-DSP | [Not Used]
SCAN-RSL | Setting of scanned image resolution
Lv.1 | Details | To set the resolution of image which is generated by scan processing.
Use case | When the scan processing performance with 1200 dpi is low
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 0 to 1 0: 600 dpi, 1: 1200 dpi
Default value | 0
JA-SBOX | Setting of linking with Advanced Box:SAM
Lv.1 | Details | To set the link with Advanced Box when iW SAM is enabled. When 1 is set, linking with Advanced Box is enabled.
Use case | When the operation restriction is cleared at the time of iW SAM
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 0 to 1 0: Disabled, 1: Enabled
Default value | 0
JA-DFAX | Setting of direct fax transmission: SAM
Lv.1 | Details | To set the direct fax transmission when iW SAM is enabled. When 1 is set, the direct fax transmission is enabled.
Use case | When the operation restriction is cleared at the time of iW SAM
Display/adj/set range | 0 to 1 0: Disabled, 1: Enabled
Default value | 0
JA-REP | Setting of TX Report with image: SAM
Lv.1 | Details | To set the TX Report with image when iW SAM is enabled. When 1 is set, the TX Report with image is enabled.
Use case | When the operation restriction is cleared at the time of iW SAM
Display/adj/set range | 0 to 1 0: Disabled, 1: Enabled
Default value | 0
JA-FREP | Setting of Fax TX Report with image: SAM
Lv.1 | Details | To set the Fax TX Report with image when iW SAM is enabled. When 1 is set, the Fax TX Report with image is enabled.
Use case | When the operation restriction is cleared at the time of iW SAM
Display/adj/set range | 0 to 1 0: Disabled, 1: Enabled
Default value | 0
JA-BOX | Setting of Inbox document operation: SAM
Lv.1 | Details | To set the operation for Inbox document at the time of iW SAM When 1 is set, the Inbox document can be operated.
Use case | When the operation restriction is cleared at the time of iW SAM
Display/adj/set range | 0 to 1 0: Disabled, 1: Enabled
Default value | 0
JA-FORM | Setting of image composition: SAM
Lv.1 | Details | To set the image composition when iW SAM is enabled. When 1 is set, the image composition is enabled.
Use case | When the operation restriction is cleared at the time of iW SAM
Display/adj/set range | 0 to 1 0: Disabled, 1: Enabled
Default value | 0
JA-PREV | Setting of preview page deletion: SAM
Lv.1 | Details | To set whether a page is deleted from the scan preview screen at the time of iW SAM When 1 is set, a page is deleted from the scan preview screen.
Use case | When the operation restriction is cleared at the time of iW SAM
Display/adj/set range | 0 to 1 0: Disabled, 1: Enabled
Default value | 0
JA-PULL | Setting of network scan: SAM
Lv.1 | Details | To set the network scan when iW SAM is enabled. When 1 is set, the network scan is enabled.
Use case | When the operation restriction is cleared at the time of iW SAM
Display/adj/set range | 0 to 1 0: Disabled, 1: Enabled
Default value | 0
JA-PDLB | Set of printer driver multi box save:SAM
Lv.1 | Details | To set whether a document can be simultaneously saved to multiple Inboxes from the printer driver at the time of iW SAM. When 1 is set, a document can be saved to multiple Inboxes from the printer driver.
Use case | When the operation restriction is cleared at the time of iW SAM
Display/adj/set range | 0 to 1 0: Disabled, 1: Enabled
Default value | 0
JA-JOBK | Setting of job merge allowance:SAM
Lv.1 | Details | To set whether merging jobs is allowed when iW SAM is enabled. When 1 is set, jobs can be merged.
Use case | When the operation restriction is cleared at the time of iW SAM
Display/adj/set range | 0 to 1 0: Disabled, 1: Enabled
Default value | 0
JA-RUI | Setting of Inbox document access: SAM
Lv.1 | Details | To set the Inbox document access from remote UI at the time of iW SAM When 1 is set, accessing to the Inbox document from remote UI is enabled.
Use case | When the operation restriction is cleared at the time of iW SAM
Display/adj/set range | 0 to 1 0: Disabled, 1: Enabled
Default value | 0
JA-WEB | Setting of Inbox document upload: SAM
Lv.1 | Details | To set the Inbox document upload with the Web browser at the time of iW SAM. When 1 is set uploading to the Inbox document with the Web Browser is enabled.
Use case | When the operation restriction is cleared at the time of iW SAM
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 0 to 1 0: Disabled, 1: Enabled
Default value | 0
EXP-CRYP | Confidential encrypt ON/OFF:add book exprt
Lv.1 | Details | To set whether to encrypt the confidential part (password part) in the Address Book when exporting the Address Book and device settings via RUI. When 0 is set, the confidential part in the Address Book is exported without encryption.
Use case | When there is a need to export password without encryption because of operation and tool
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Caution | Be sure not to allow the user to execute export without encryption because of security concern.
Display/adj/set range | 0 to 1 0: OFF, 1: ON
Default value | 1
SLEEP1SW | Power supply when shifting to SLEEP1
Lv.1 | Details | When shifting to SLEEP1 mode, the power stops to be supplied, so it takes time to activate after a job is received. When 1 is set, the power keeps to be supplied even after shifting to SLEEP1 mode, so the activation of job processing becomes earlier.
Use case | Upon user's request (when job processing after shifting to SLEEP1 is slow)
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 0 to 1 0: OFF, 1: ON
Default value | 0
EZY-SCRP | Set simple certify printing mode
Lv.1 | Details | The following operations are performed for the certify printing. 1. The secure print is available without the pass word by certifying the prescribed pass word automatically. 2. The job only to perform secure printing is acceptable. 3. The items 10 min, 20 min and 30 min are added to the automatic erase time of the secure job.
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 0 to 1 0: OFF, 1: ON
Default value | 0
DMN-MTCH | Secure print domain mode
Lv.1 | Details | To wide an application range of my job by flexing the relation condition of the domain
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 0 to 1 0: OFF, 1: ON
Default value | 1