Cautions

| Print out this category

Cautions
Concurrent use of Updater functions
Multiple users cannot use Updater functions on a device concurrently by using it together with Remote UI.
Coexistence of Remote UI and other tools
Users logged in SMS (Service Management Service) are unable to use Update functions from Remote UI.
Using Updater function from Remote UI
Upon the following operations done, Updater functions are suspended from Remote UI for certain duration.
When a user exits Web browser without clicking [Portal] or [Log Out] button in the setting of Remote Login Service via SMS
When a user exits Web browser without clicking [Portal] button in the setting of not to use Remote Login Service via SMS.
When a user exits Web browser without clicking [Log out from SMS] or [To Remote UI] button.
﻿Wait for EOJ (end of job) Function
Firmware update will be triggered only after the following jobs are completed.
This is the Updater-specific specification.

Job/Function type | Receiving | Printing | Queued print jobs | Sending | Queued send jobs
COPY | - | Wait for EOJ | Wait for EOJ | - | -
PRINT | Wait for EOJ (end of job) | Wait for EOJ | Wait for EOJ | - | -
FAX | Wait for EOJ | Wait for EOJ | Wait for EOJ | Wait for EOJ | Wait for EOJ
I-FAX Receipt | Cancel processing to trigger update * | Wait for EOJ | Wait for EOJ | Wait for EOJ | Wait for EOJ
Report Print | - | Wait for EOJ | Wait for EOJ | - | -
SEND | - | - | - | Cancel processing to trigger update * | Cancel processing to trigger update *

*The data are guaranteed even if cut off in the middle of a job.It becomes the recovery object after the device reboot and carry out send / reception again.
Even during transfer, Pull SCAN job processing is cancelled soon after scanning is completed.
Firmware update is cancelled if the jobs are not completed within 10 minutes. If this occurs, the error code, 8x001106, will be returned (different numbers will be shown for x depending on the execution modes).
Firmware update is executed if the jobs stated above are not in the queue.
Follow the shutdown sequence to reboot the device after the firmware is updated.