CST

| Print out this category

CST

COPIER>OPTION>CST
U1-NAME | Dis/hide of ppr name in ppr size groupU1
Lv.2 | Details | To set whether to display or hide paper name at paper size group U1 detection.
Use case | Upon user's request
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 0 to 1 0: Hide, 1: Display
Default value | 0
U2-NAME | Dis/hide of ppr name in ppr size groupU2
Lv.2 | Details | To set whether to display or hide paper name at paper size group U2 detection.
Use case | Upon user's request
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 0 to 1 0: Hide, 1: Display
Default value | 0
U3-NAME | Dis/hide of ppr name in ppr size groupU3
Lv.2 | Details | To set whether to display or hide paper name at paper size group U3 detection.
Use case | Upon user's request
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 0 to 1 0: Hide, 1: Display
Default value | 0
U4-NAME | Dis/hide of ppr name in ppr size groupU4
Lv.2 | Details | To set whether to display or hide paper name at paper size group U4 detection.
Use case | Upon user's request
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 0 to 1 0: Hide, 1: Display
Default value | 0
ENV1 | Registration of envelope cassette size (ENV1)
Lv.1 | Details | Set the paper size for the envelope cassette.
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 21: ISO-C5, 22: COM10, 23: MONARCH, 24: DL, 25: ISO-B5, 26: Youkei No. 4
Default value | 21
ENV2 | Registration of envelope cassette size (ENV2)
Lv.1 | Details | Set the paper size for the envelope cassette.
Display/adj/set range | 21: ISO-C5, 22: COM10, 23: MONARCH, 24: DL, 25: ISO-B5, 26: Youkei No. 4
Default value | 21
CST1-P1 | Setting of Cassette 1 paper size
Lv.1 | Details | To set the paper size used in Cassette 1.
Use case | Upon user's request
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Caution | Be sure to match with the hardware setting size.
Display/adj/set range | 0 to 1 0: A5R, 1: STMTR
Default value | USA: 1, Countries other than USA: 0
Related user mode | Preferences> Paper Settings> Paper Settings> A5R/STMTR Original Selection
CST1-P2 | Setting of Cassette 1 paper size
Lv.1 | Details | To set the paper size used in Cassette 1.
Use case | Upon user's request
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Caution | Be sure to match with the hardware setting size.
Display/adj/set range | 0 to 1 0: B5, 1: EXEC
Default value | USA: 1, Countries other than USA: 0
Related user mode | Preferences> Paper Settings> Paper Settings> B5/EXEC Original Selection
CST2-P1 | Setting of Cassette 2 paper size
Lv.1 | Details | To set the paper size used in Cassette 2.
Use case | Upon user's request
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Caution | Be sure to match with the hardware setting size.
Display/adj/set range | 0 to 1 0: A5R, 1: STMTR
Default value | USA: 1, Countries other than USA: 0
Related user mode | Preferences> Paper Settings> Paper Settings> A5R/STMTR Original Selection
CST2-P2 | Setting of Cassette 2 paper size
Lv.1 | Details | To set the paper size used in Cassette 2.
Use case | Upon user's request
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Caution | Be sure to match with the hardware setting size.
Display/adj/set range | 0 to 1 0: B5, 1: EXEC
Default value | USA: 1, Countries other than USA: 0
Related user mode | Preferences> Paper Settings> Paper Settings> B5/EXEC Original Selection
CST3-P1 | Setting of Cassette 3 paper size
Lv.1 | Details | To set the paper size used in Cassette 3.
Use case | Upon user's request
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Caution | Be sure to match with the hardware setting size.
Display/adj/set range | 0 to 1 0: A5R, 1: STMTR
Default value | USA: 1, Countries other than USA: 0
Related user mode | Preferences> Paper Settings> Paper Settings> A5R/STMTR Original Selection
CST3-P2 | Setting of Cassette 3 paper size
Lv.1 | Details | To set the paper size used in Cassette 3.
Use case | Upon user's request
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Caution | Be sure to match with the hardware setting size.
Display/adj/set range | 0 to 1 0: B5, 1: EXEC
Default value | USA: 1, Countries other than USA: 0
Related user mode | Preferences> Paper Settings> Paper Settings> B5/EXEC Original Selection
CST4-P1 | Setting of Cassette 4 paper size
Lv.1 | Details | To set the paper size used in Cassette 4.
Use case | Upon user's request
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Caution | Be sure to match with the hardware setting size.
Display/adj/set range | 0 to 1 0: A5R, 1: STMTR
Default value | USA: 1, Countries other than USA: 0
Related user mode | Preferences> Paper Settings> Paper Settings> A5R/STMTR Original Selection
CST4-P2 | Setting of Cassette 4 paper size
Lv.1 | Details | To set the paper size used in Cassette 4.
Use case | Upon user's request
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Caution | Be sure to match with the hardware setting size.
Display/adj/set range | 0 to 1 0: B5, 1: EXEC
Default value | USA: 1, Countries other than USA: 0
Related user mode | Preferences> Paper Settings> Paper Settings> B5/EXEC Original Selection
CST1-U1 | Set Cst1 overseas special ppr category 1
Lv.1 | Details | To set the overseas special paper category 1 used in Cassette 1.
Use case | Upon user's request
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 0 to 43 0: Special paper is not used, 1 to 23: Not used, 24: FLSP, 25: A-FLSP, 26: OFI, 27: E-OFI, 28 to 29: Not used, 30: A-LTRR, 31 to 32: Not used, 33: A-LGL, 34: G-LGL, 35: Not used, 36: A-OFI, 37: M-OFI, 38 to 41: Not used, 42: FA4, 43: FB4 (FLSP-R)
Default value | 0
CST1-U2 | Set Cst1 overseas special ppr category 2
Lv.1 | Details | To set the overseas special paper category 2 used in Cassette 1.
Use case | Upon user's request
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 0 to 34 0: Special paper is not used, 1 to 22: Not used, 23: K-LGLR, 24 to 31: Not used, 32: G-LTRR, 33 to 34: Not used
Default value | 0
CST1-U3 | Set Cst1 overseas special ppr category 3
Lv.1 | Details | To set the overseas special paper category 3 used in Cassette 1.
Use case | Upon user's request
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 0 to 31 0: Special paper is not used, 1 to 21: Not used, 22: K-LGL, 23 to 28: Not used, 29:A-LTR, 30: Not used, 31: G-LTR
Default value | 0
CST1-U4 | Set Cst1 overseas special ppr category 4
Lv.1 | Details | To set the overseas special paper category 4 used in Cassette 1.
Use case | Upon user's request
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 0 to 28 0: Special paper is not used, 1 to 27: Not used, 28: B-OFI
Default value | 0
CST2-U1 | Set Cst2 overseas special ppr category 1
Lv.1 | Details | To set the overseas special paper category 1 used in Cassette 2.
Use case | Upon user's request
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 0 to 43 0: Special paper is not used, 1 to 23: Not used, 24: FLSP, 25: A-FLSP, 26: OFI, 27: E-OFI, 28 to 29: Not used, 30: A-LTRR, 31 to 32: Not used, 33: A-LGL, 34: G-LGL, 35: Not used, 36: A-OFI, 37: M-OFI, 38 to 41: Not used, 42: FA4, 43: FB4 (FLSP-R)
Default value | 0
CST2-U2 | Set Cst2 overseas special ppr category 2
Lv.1 | Details | To set the overseas special paper category 2 used in Cassette 2.
Use case | Upon user's request
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 0 to 34 0: Special paper is not used, 1 to 22: Not used, 23: K-LGLR, 24 to 31: Not used, 32: G-LTRR, 33 to 34: Not used
Default value | 0
CST2-U3 | Set Cst2 overseas special ppr category 3
Lv.1 | Details | To set the overseas special paper category 3 used in Cassette 2.
Use case | Upon user's request
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 0 to 31 0: Special paper is not used, 1 to 21: Not used, 22: K-LGL, 23 to 28: Not used, 29:A-LTR, 30: Not used, 31: G-LTR
Default value | 0
CST2-U4 | Set Cst2 overseas special ppr category 4
Lv.1 | Details | To set the overseas special paper category 4 used in Cassette 2.
Use case | Upon user's request
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 0 to 28 0: Special paper is not used, 1 to 27: Not used, 28: B-OFI
Default value | 0
CST3-U1 | Set Cst3 overseas special ppr category 1
Lv.1 | Details | To set the overseas special paper category 1 used in Cassette 3.
Use case | Upon user's request
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 0 to 43 0: Special paper is not used, 1 to 23: Not used, 24: FLSP, 25: A-FLSP, 26: OFI, 27: E-OFI, 28 to 29: Not used, 30: A-LTRR, 31 to 32: Not used, 33: A-LGL, 34: G-LGL, 35: Not used, 36: A-OFI, 37: M-OFI, 38 to 41: Not used, 42: FA4, 43: FB4 (FLSP-R)
Default value | 0
CST3-U2 | Set Cst3 overseas special ppr category 2
Lv.1 | Details | To set the overseas special paper category 2 used in Cassette 3.
Use case | Upon user's request
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 0 to 34 0: Special paper is not used, 1 to 22: Not used, 23: K-LGLR, 24 to 31: Not used, 32: G-LTRR, 33 to 34: Not used
Default value | 0
CST3-U3 | Set Cst3 overseas special ppr category 3
Lv.1 | Details | To set the overseas special paper category 3 used in Cassette 3.
Use case | Upon user's request
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 0 to 31 0: Special paper is not used, 1 to 21: Not used, 22: K-LGL, 23 to 28: Not used, 29:A-LTR, 30: Not used, 31: G-LTR
Default value | 0
CST3-U4 | Set Cst3 overseas special ppr category 4
Lv.1 | Details | To set the overseas special paper category 4 used in Cassette 3.
Use case | Upon user's request
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 0 to 28 0: Special paper is not used, 1 to 27: Not used, 28: B-OFI
Default value | 0
CST4-U1 | Set Cst4 overseas special ppr category 1
Lv.1 | Details | To set the overseas special paper category 1 used in Cassette 4.
Use case | Upon user's request
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 0 to 43 0: Special paper is not used, 1 to 23: Not used, 24: FLSP, 25: A-FLSP, 26: OFI, 27: E-OFI, 28 to 29: Not used, 30: A-LTRR, 31 to 32: Not used, 33: A-LGL, 34: G-LGL, 35: Not used, 36: A-OFI, 37: M-OFI, 38 to 41: Not used, 42: FA4, 43: FB4 (FLSP-R)
Default value | 0
CST4-U2 | Set Cst4 overseas special ppr category 2
Lv.1 | Details | To set the overseas special paper category 2 used in Cassette 4.
Use case | Upon user's request
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 0 to 34 0: Special paper is not used, 1 to 22: Not used, 23: K-LGLR, 24 to 31: Not used, 32: G-LTRR, 33 to 34: Not used
Default value | 0
CST4-U3 | Set Cst4 overseas special ppr category 3
Lv.1 | Details | To set the overseas special paper category 3 used in Cassette 4.
Use case | Upon user's request
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 0 to 31 0: Special paper is not used, 1 to 21: Not used, 22: K-LGL, 23 to 28: Not used, 29:A-LTR, 30: Not used, 31: G-LTR
Default value | 0
CST4-U4 | Set Cst4 overseas special ppr category 4
Lv.1 | Details | To set the overseas special paper category 4 used in Cassette 4.
Use case | Upon user's request
Adj/set/operate method | 1) Enter the setting value, and then press OK key. 2) Turn OFF/ON the main power switch.
Display/adj/set range | 0 to 28 0: Special paper is not used, 1 to 27: Not used, 28: B-OFI
Default value | 0