Operation Procedure Using Ping

| Print out this category

Operation Procedure Using Ping
1) Ask the network administrator at the user’s site to write down the IP address of the PC that is connected to the network.
2) [Additional Functions] > [Configuration] > [Network] > [TCP/IP Setting] > [IPv4 setting] > [Ping Command]; and enter the IP address of the PC with the numeric keypad and press Execute key.
The network is properly connected if the message say "Response from the host".
If the message say "No response from the host", check the following.
NOTE:
The IP address of the PC can be checked by the following procedure:
Select the following on a Windows PC: Start > Program > Accessory > Command
Prompt; and enter “ipconfig” and press Enter key to display information of the IP address.