Inner Finisher-D1/Inner Hole Puncher-A1 SORTER>P001 to P015

| Print out this category

Inner Finisher-D1/Inner Hole Puncher-A1 SORTER>P001 to P015

Address | bit | Name | Symbol | Remarks
P001 | 7 | Entrance Sensor | S1 | 1:Paper presence
6 | Grip Arm Sensor | S13 | 0: HP
5 | Not used |  |
4 | Not used |  |
3 | Not used |  |
2 | For R&D use |  |
1 | For R&D use |  |
0 | Not used |  |
P002 | 7 | Not used |  |
6 | Not used |  |
5 | Not used |  |
4 | Not used |  |
3 | Not used |  |
2 | Not used |  |
1 | Not used |  |
0 | Not used |  |
P003 | 7 | Not used |  |
6 | Not used |  |
5 | Not used |  |
4 | Not used |  |
3 | Not used |  |
2 | Not used |  |
1 | Not used |  |
0 | Not used |  |
P004 | 7 | Punch Solenoid Sensor | SR1 | 1: ON
6 | Punch Path Sensor | SR3 | 1:Paper presence
5 | For R&D use |  |
4 | For R&D use |  |
P005 | 7 | Not used |  |
6 | Scrap Full Detector PCB | PCB13 | 1: Full
5 | Photosensor PCB (Rear Edge of Paper) | PCB11 | 1:Paper presence
4 | Punch HP Sensor | SR5 | 1: HP
3 | Additional Tray Clock Sensor | S23 |
2 | Stack Tray Clock Sensor | S14 |
1 | Stapler Move HP Sensor | S10 | 1:Paper presence
0 | Stapler HP Sensor | S18 | 1: HP
P006 | 7 | Punch Clock Sensor | SR4 |
6 | Not used |  |
5 | Entrance Roller Release /Stopper HP Sensor | S5 | 0: HP
4 | Gripper Unit HP Sensor | S7 | 0: Evacuation
3 | Shift Roller Release Sensor | S3 | 1: Release
2 | Shift roller HP Sensor | S2 | 0: HP
1 | For R&D use |  |
0 | Not used |  |
P007 | 7 | Additional Tray Upper/Lower Lmit Sensor | S21 | 1: Upper or lower limit
6 | Not used |  |
5 | Not used |  |
4 | Not used |  |
3 | Not used |  |
2 | Not used |  |
1 | Not used |  |
0 | For R&D use |  |
P008 | 7 | Not used |  |
6 | Not used |  |
5 | Not used |  |
4 | Not used |  |
3 | Not used |  |
2 | For R&D use |  |
1 | For R&D use |  |
0 | Additional Tray Paper Sensor | S22 | 1:Paper presence
P009 | 5 | Release Sensor | SR2 | 1: Release
4 | Not used |  |
3 | Not used |  |
2 | Not used |  |
1 | Puncher Unit Connect Detection |  | 0: Connect
0 | Not used |  |
P010 | 7 | Not used |  |
6 | Not used |  |
5 | Not used |  |
4 | Not used |  |
3 | Not used |  |
2 | Not used |  |
1 | Not used |  |
0 | Not used |  |
P011 | 7 | Not used |  |
6 | Not used |  |
5 | Not used |  |
4 | Not used |  |
3 | Not used |  |
2 | Not used |  |
1 | Not used |  |
0 | Not used |  |
P012 | 7 | For R&D use |  |
6 | For R&D use |  |
5 | For R&D use |  |
4 | For R&D use |  |
3 | Stack Tray Paper Sensor | S15 | 1:Paper presence
2 | Stack Tray Lower Limit Sensor | S17 | 1: Lower limit
1 | Stack Tray Middle Sensor | S16 | 1:Paper presence
0 | Not used |  |
P013 | 7 | Processing Tray Sensor | S6 | 1:Paper presence
6 | Stapler Safety Switch | SW2 | 1: ON
5 | Not used |  |
4 | Gripper Stapler Connection Sensor | S9 | 1: Connection
3 | Not used |  |
2 | Front Fan Lock Signal | FM1 | 1: Lock
1 | Rear fan Lock Signal | FM2 | 1: Lock
0 | Not used |  |
P014 | 7 | For R&D use |  |
6 | Not used |  |
5 | Paper Surface Sensor 2 | S12 | 1:Paper presence
4 | Paper Surface Sensor 1 | S11 | 1:Paper presence
3 | Stapler Edging Sensor | S19 | 1: Edging
2 | Stapler Sensor | S20 | 1: No needle
1 | Not used |  |
0 | Front Cover Switch | SW1 | 1: Open
P015 | 3 | Not used |  |
2 | Not used |  |
1 | Not used |  |
0 | Not used |  |