Relation between SST and USB memory Storage Device

| Print out this category

Version Upgrade using USB memory Storage Device
Relation between SST and USB memory Storage Device
When using the USB memory storage device storage device for version upgrade, the system software should be copied to the USB memory storage device storage device. By inserting the USB memory storage device storage device to the slot of the machine, the system software can be upgraded.
The figure below shows the relation between SST and USB memory storage device storage device.
When downloading the system software, enter any of Download modes below.
Normal mode (recommended)
Select COPIER > FUNCTION > SYSTEM > Download in Service mode and press [OK].
Safe mode (only when any system error occurs or the machine is unable to start normally; turn ON the main power switch by pressing 2 and 8 keys simultaneously on the numeric keypad)
Downloading System Software
Copy the system software from SST to the USB memory storage device storage device.
Right after download from the USB memory storage device storage device, the system software is stored in the temporary memory space in HDD.
The system software is written in the system memory area, Boot area and Flash ROM upon the machine restarted.
When the writing process is successfully completed, the machine is automatically restarted with the new version of the system software.