Starting in Safe Mode

| Print out this category

Starting in Safe Mode
1) Startup level 2 of [ SERVICE MODE ].
2) Press [ COPIER ] > [ Option ] > [ USER ].
3) Press or button for several times until [ MEAPSAFE ] is shown. Click [ MEAPSAFE ].
4) Press the 1 key on the control panel keypad to change the setting to '1'; then, click [ OK ] button.
5) Check that the notation ‘MPSF’ has appeared in the upper left corner of the screen; then, restart the device.
Note:
If accessed to SMS in MEAP SAFE mode, the device started mode is shown on the title bar of the browser.
Example of display when starting in MEAP SAFE mode:
Service Management Service : <Device Name>:<Product Name>: Safe Mode
WARNING :
If the device has been started in the MEAP SAFE mode, all MEAP applications stop and the status becomes "Installed".
This status remains unchanged even if the MEAP SAFE mode is cancelled and the device is started again in normal mode. It is therefore necessary to access SMS after normal startup, and start the MEAP application.