Data Encryption Mechanism

| Print out this category

Data Encryption Mechanism
The encryption PCB receives signals transmitted from the Main Controller PCB, and encrypts and saves them in the HDD. The encryption PCB receives the encrypted data saved in the HDD to decode and send them to the Main Controller PCB.
The encryption PCB can be configured with a HDD and an encryption/ mirroring PCB, or with 2 HDDs and an Encryption/Mirroring PCB.