BLANK

| Print out this category

BLANK

COPIER>ADJUST>BLANK
BLANK-T | Adjustment of leading edge margin
Lv.1 | Details | To adjust the margin on the leading edge of paper. As the value is incremented by 1, the margin is increased toward the center of the paper by 1 pixel (0.0212 mm).
Use case | - When reducing the margin upon user's request - When enlarging the margin for transfer separation/fixing separation
Adj/set/operate method | Enter the setting value, and then press OK key.
Caution | Do not use this at the normal service. After the setting value is changed, write the changed value in the service label.
Display/adj/set range | -128 to 127
BLANK-B | Adjustment of trailing edge margin
Lv.1 | Details | To adjust the margin on the trailing edge of paper. As the value is incremented by 1, the margin is increased toward the center of the paper by 1 pixel (0.0212 mm).
Use case | - When reducing the margin upon user's request - When enlarging the margin for transfer separation/fixing separation
Adj/set/operate method | Enter the setting value, and then press OK key.
Caution | After the setting value is changed, write the changed value in the service label.
Display/adj/set range | -128 to 127