DRBL-2

| Print out this category

DRBL-2

COPIER>COUNTER>DRBL-2
DF-PU-RL | Pickup Roller parts counter: DADF
Lv.1 | Details | 1st line: Total counter value from the previous replacement 2nd line: Estimated life
Use case | When checking the consumption level of parts/replacing the parts
Adj/set/operate method | To clear the counter value: Select the item, and then press Clear key. To change the estimated life: Select the item, enter the value, and then press OK key.
Caution | Clear the counter value after replacement.
Display/adj/set range | 0 to 99999999
Unit | Number of sheets
Default value | 0
Supplement/memo | Regardless of the read mode (1-sided/2-sided), the counter is advanced every time a sheet is fed.
DF-SP-PD |  | Separation Pad parts counter: DADF
Lv.1 | Details | 1st line: Total counter value from the previous replacement 2nd line: Estimated life
Use case | When checking the consumption level of parts/replacing the parts
Adj/set/operate method | To clear the counter value: Select the item, and then press Clear key. To change the estimated life: Select the item, enter the value, and then press OK key.
Caution | Clear the counter value after replacement.
Display/adj/set range | 0 to 99999999
Unit | Number of sheets
Default value | 0
Supplement/memo | Regardless of the read mode (1-sided/2-sided), the counter is advanced every time a sheet is fed.
LNT-TAP1 | Dust Removal Sheet 1 counter: DADF
Lv.1 | Details | Dust-colleting 1st line: Total counter value from the previous replacement 2nd line: Estimated life
Use case | When checking the consumption level of parts/replacing the parts
Adj/set/operate method | To clear the counter value: Select the item, and then press Clear key. To change the estimated life: Select the item, enter the value, and then press OK key.
Caution | Clear the counter value after replacement.
Display/adj/set range | 0 to 99999999
Unit | Number of sheets
Default value | 0
Supplement/memo | Regardless of the read mode (1-sided/2-sided), the counter is advanced every time a sheet is fed.
STAMP | Stamp parts counter: DADF
Lv.1 | Details | To display the estimated life and parts counter of DADF stamp. 1st line: Total counter value from the previous replacement 2nd line: Estimated life to be entered by operator
Use case | At replacement
Adj/set/operate method | To clear the counter value: Select the item, and then press Clear key. To change the estimated life: Select the item, enter the value, and then press OK key.
Caution | Clear the counter value after replacement.
Display/adj/set range | 0 to 99999999
Unit | Number of sheets
Default value | 0
PD-PU-RL | Pickup Roller parts counter: Deck
Lv.1 | Details | Pickup Roller (Front/Rear) of Paper Deck/POD Deck Lite/Multi Deck (Upper) 1st line: Total counter value from the previous replacement 2nd line: Estimated life
Use case | When checking the consumption level of parts/replacing the parts
Adj/set/operate method | To clear the counter value: Select the item, and then press Clear key. To change the estimated life: Select the item, enter the value, and then press OK key.
Caution | Clear the counter value after replacement.
Display/adj/set range | 0 to 99999999
Unit | Number of sheets
Default value | 0
PD-SP-RL | Separation Roller parts counter: Deck
Lv.1 | Details | Separation Roller of Paper Deck/POD Deck Lite/Multi Deck (Upper) 1st line: Total counter value from the previous replacement 2nd line: Estimated life
Use case | When checking the consumption level of parts/replacing the parts
Adj/set/operate method | To clear the counter value: Select the item, and then press Clear key. To change the estimated life: Select the item, enter the value, and then press OK key.
Caution | Clear the counter value after replacement.
Display/adj/set range | 0 to 99999999
Unit | Number of sheets
Default value | 0
PD-FD-RL | Feed Roller parts counter: Deck
Lv.1 | Details | Feed Roller of Paper Deck/POD Deck Lite/Multi Deck (Upper) 1st line: Total counter value from the previous replacement 2nd line: Estimated life
Use case | When checking the consumption level of parts/replacing the parts
Adj/set/operate method | To clear the counter value: Select the item, and then press Clear key. To change the estimated life: Select the item, enter the value, and then press OK key.
Caution | Clear the counter value after replacement.
Display/adj/set range | 0 to 99999999
Unit | Number of sheets
Default value | 0
C3-PU-RL | Cassette 3 Pickup Roller parts counter
Lv.1 | Details | 1st line: Total counter value from the previous replacement 2nd line: Estimated life
Use case | When checking the consumption level of parts/replacing the parts
Adj/set/operate method | To clear the counter value: Select the item, and then press Clear key. To change the estimated life: Select the item, enter the value, and then press OK key.
Caution | Clear the counter value after replacement.
Display/adj/set range | 0 to 99999999
Unit | Number of sheets
Default value | 0
C3-SP-RL | Cassette 3 Separation Roller parts counter
Lv.1 | Details | 1st line: Total counter value from the previous replacement 2nd line: Estimated life
Use case | When checking the consumption level of parts/replacing the parts
Adj/set/operate method | To clear the counter value: Select the item, and then press Clear key. To change the estimated life: Select the item, enter the value, and then press OK key.
Caution | Clear the counter value after replacement.
Display/adj/set range | 0 to 99999999
Unit | Number of sheets
Default value | 0
C3-FD-RL | Cassette 3 Feed Roller parts counter
Lv.1 | Details | 1st line: Total counter value from the previous replacement 2nd line: Estimated life
Use case | When checking the consumption level of parts/replacing the parts
Adj/set/operate method | To clear the counter value: Select the item, and then press Clear key. To change the estimated life: Select the item, enter the value, and then press OK key.
Caution | Clear the counter value after replacement.
Display/adj/set range | 0 to 99999999
Unit | Number of sheets
Default value | 0
C4-PU-RL | Cassette 4 Pickup Roller parts counter
Lv.1 | Details | 1st line: Total counter value from the previous replacement 2nd line: Estimated life
Use case | When checking the consumption level of parts/replacing the parts
Adj/set/operate method | To clear the counter value: Select the item, and then press Clear key. To change the estimated life: Select the item, enter the value, and then press OK key.
Caution | Clear the counter value after replacement.
Display/adj/set range | 0 to 99999999
Unit | Number of sheets
Default value | 0
C4-SP-RL | Cassette 4 Separation Roller parts counter
Lv.1 | Details | 1st line: Total counter value from the previous replacement 2nd line: Estimated life
Use case | When checking the consumption level of parts/replacing the parts
Adj/set/operate method | To clear the counter value: Select the item, and then press Clear key. To change the estimated life: Select the item, enter the value, and then press OK key.
Caution | Clear the counter value after replacement.
Display/adj/set range | 0 to 99999999
Unit | Number of sheets
Default value | 0
C4-FD-RL | Cassette 4 Feed Roller parts counter
Lv.1 | Details | 1st line: Total counter value from the previous replacement 2nd line: Estimated life
Use case | When checking the consumption level of parts/replacing the parts
Adj/set/operate method | To clear the counter value: Select the item, and then press Clear key. To change the estimated life: Select the item, enter the value, and then press OK key.
Caution | Clear the counter value after replacement.
Display/adj/set range | 0 to 99999999
Unit | Number of sheets
Default value | 0
SORT | Finisher sort path feed paper counter
| Use case | When checking the consumption level of parts
Adj/set/operate method | To clear the counter value: Select the item, and then press Clear key. To change the estimated life: Select the item, enter the value, and then press OK key.
Caution | Clear the counter value after replacement.
Display/adj/set range | 0 to 99999999
Unit | Number of sheets
Default value | 0
FIN-STPR | Stapler parts counter: Inner/External Finisher
Lv.1 | Details | Stapler Unit 1st line: Total counter value from the previous replacement 2nd line: Estimated life
Use case | When checking the consumption level of parts/replacing the parts
Adj/set/operate method | To clear the counter value: Select the item, and then press Clear key. To change the estimated life: Select the item, enter the value, and then press OK key.
Caution | Clear the counter value after replacement.
Display/adj/set range | 0 to 99999999
Unit | Number of times
Default value | 0
SADDLE | Saddle feed path feed paper counter: Saddle Finisher
| Use case | When checking the consumption level of parts
Adj/set/operate method | To clear the counter value: Select the item, and then press Clear key. To change the estimated life: Select the item, enter the value, and then press OK key.
Caution | Clear the counter value after replacement.
Display/adj/set range | 0 to 99999999
Unit | Number of sheets
Default value | 0
SDL-STPL | Saddle staple unit operation counter: Saddle Finisher
Lv.1 | Details | 1st line: Total counter value from the previous replacement 2nd line: Estimated life
Use case | When checking the consumption level of parts/replacing the parts
Adj/set/operate method | To clear the counter value: Select the item, and then press Clear key. To change the estimated life: Select the item, enter the value, and then press OK key.
Caution | Clear the counter value after replacement.
Display/adj/set range | 0 to 99999999
Unit | Number of sheets
Default value | 0
PUNCH | Punch unit operation counter: Puncher
Lv.1 | Details | 1st line: Total counter value from the previous replacement 2nd line: Estimated life
Use case | When checking the consumption level of parts/replacing the parts
Adj/set/operate method | To clear the counter value: Select the item, and then press Clear key. To change the estimated life: Select the item, enter the value, and then press OK key.
Caution | Clear the counter value after replacement.
Display/adj/set range | 0 to 99999999
Unit | Number of sheets
Default value | 0
FN-BFFRL | Buffer Roller parts counter: External Finisher
Lv.1 | Details | 1st line: Total counter value from the previous replacement 2nd line: Estimated life
Use case | When checking the consumption level of parts/replacing the parts
Adj/set/operate method | To clear the counter value: Select the item, and then press Clear key. To change the estimated life: Select the item, enter the value, and then press OK key.
Caution | Clear the counter value after replacement.
Display/adj/set range | 0 to 99999999
Default value | 0
ENT-STC | Inlet Static Eliminator prts cntr: Inner/External Finisher
Lv.1 | Details | 1st line: Total counter value from the previous replacement 2nd line: Estimated life
Use case | When checking the consumption level of parts/replacing the parts
Adj/set/operate method | To clear the counter value: Select the item, and then press Clear key. To change the estimated life: Select the item, enter the value, and then press OK key.
Caution | Clear the counter value after replacement.
Display/adj/set range | 0 to 99999999
Unit | Number of sheets
Default value | 0
DL-STC | Delivery Static Eliminator prts cntr: Inner/External Finisher
Lv.1 | Details | 1st line: Total counter value from the previous replacement 2nd line: Estimated life
Use case | When checking the consumption level of parts/replacing the parts
Adj/set/operate method | To clear the counter value: Select the item, and then press Clear key. To change the estimated life: Select the item, enter the value, and then press OK key.
Caution | Clear the counter value after replacement.
Display/adj/set range | 0 to 99999999
Unit | Number of sheets
Default value | 0
OFST-RL | Offset roller parts counter: Inner Finisher
Lv.1 | Details | 1st line: Total counter value from the previous replacement 2nd line: Estimated life
Use case | When checking the consumption level of parts/replacing the parts
Adj/set/operate method | To clear the counter value: Select the item, and then press Clear key. To change the estimated life: Select the item, enter the value, and then press OK key.
Caution | Clear the counter value after replacement.
Display/adj/set range | 0 to 99999999
Unit | Number of sheets
Default value | 0
RET-RL | Return roller parts counter: External Finisher
Lv.1 | Details | 1st line: Total counter value from the previous replacement 2nd line: Estimated life
Use case | When checking the consumption level of parts/replacing the parts
Adj/set/operate method | To clear the counter value: Select the item, and then press Clear key. To change the estimated life: Select the item, enter the value, and then press OK key.
Caution | Clear the counter value after replacement.
Display/adj/set range | 0 to 99999999
Unit | Number of sheets
Default value | 0
SWG-STC | Swing Middle Static Eliminator prts cntr: External Finisher
Lv.1 | Details | 1st line: Total counter value from the previous replacement 2nd line: Estimated life
Use case | When checking the consumption level of parts/replacing the parts
Adj/set/operate method | To clear the counter value: Select the item, and then press Clear key. To change the estimated life: Select the item, enter the value, and then press OK key.
Caution | Clear the counter value after replacement.
Display/adj/set range | 0 to 99999999
Unit | Number of sheets
Default value | 0