﻿Removing the Cassette Pickup Unit 1

| Print out this category

Pickup Feed System
Removing the Cassette Pickup Unit 1
1) Draw out the cassette.
2) Open the right cover.
3) Remove the stopper cover.
1 screw
4) Remove the right cover (lower).(only when the cassette feeding unit is not installed)
5) Remove the rear right cover (lower).(Reference)
6) Remove the handle cover.
7) ﻿Remove the front right cover (lower)
3 screws
2 claws
8) Remove the connection cable.
2 connector
4 clamps
9) Remove the cassette pickup unit 1.
5 screws