Backup

| Print out this category

Backup
[5]: Backup
CAUTION:
This function includes R&D review.
Do not usually use it other than the following function.
When the data is sent to the USB memory device:
USB memory where the system software for this machine has been registered using the SST.
Operation procedure
1) Enter download mode.
2) Connect the USB memory storage device to the USB port.
3) Press the key on the Control Panel.
[5] -> [0]
4) SRAM backup of Main Controller PCB2.
[4] ServicePrint -> Save the service data which P-PRINT output to paper with a text format.
[6] SRAM(HDD) -> Save it to the Host Machine HDD
[7] SRAM(USB) -> Save it in USB memory.