Related service modes

| Print out this category

Related service modes
COPIER > OPTION > FNC-SW > PSWD-SW (Level1)
Set password type for transition to service mode.
<Setting range>
0: No password (default)
1: Service engineer
2: System administrator and Service engineer.
COPIER > OPTION > FNC-SW > SM-PSWD (Level2)
Password for service engineer for transition to service mode.
<Setting range>

To reinforce the security, change the password from a default.

******** (eight digit numeral) [default: 11111111]
After the above setting, to enter Service Mode, enter password screen will appear.
1) Additional Functions > System Settings > System Manager Settings > enter System Manager ID > enter System Password Settings > press OK button.
2) After entering the password for service technician (Service mode: COPIER > Option > FNC-SW > SM-PSWD), press OK button.
MEMO :
If Service Engineer’s password is forgotten, password function is cancelable by using
Service Support Tool (SST).